3GPP TS 36.101 V10.33.0 (2022-09)

Technical Specification

3rd Generation Partnership Project;

Technical Specification Group Radio Access Network;

Evolved Universal Terrestrial Radio Access (E-UTRA);

User Equipment (UE) radio transmission and reception

(Release 10)

 

The present document has been developed within the 3rd Generation Partnership Project (3GPP TM) and may be further elaborated for the purposes of 3GPP.  
The present document has not been subject to any approval process by the 3GPPOrganizational Partners and shall not be implemented.   
This Specification is provided for future development work within 3GPPonly. The Organizational Partners accept no liability for any use of this Specification.  
Specifications and reports for implementation of the 3GPP TM system should be obtained via the 3GPP Organizational Partners' Publications Offices.

***3GPP***

Postal address

3GPP support office address

650 Route des Lucioles - Sophia Antipolis

Valbonne - FRANCE

Tel.: +33 4 92 94 42 00 Fax: +33 4 93 65 47 16

Internet

http://www.3gpp.org

***Copyright Notification***

No part may be reproduced except as authorized by written permission.  
The copyright and the foregoing restriction extend to reproduction in all media.

© 2022, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

All rights reserved.

UMTS™ is a Trade Mark of ETSI registered for the benefit of its members

3GPP™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners  
LTE™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners

GSM® and the GSM logo are registered and owned by the GSM Association

Contents

Foreword 14

1 Scope 15

2 References 15

3 Definitions, symbols and abbreviations 15

3.1 Definitions 15

3.2 Symbols 16

3.3 Abbreviations 18

4 General 19

4.1 Relationship between minimum requirements and test requirements 19

4.2 Applicability of minimum requirements 19

4.3 Void 19

4.3A Applicability of minimum requirements (CA, UL-MIMO) 19

4.4 RF requirements in later releases 20

5 Operating bands and channel arrangement 20

5.1 General 20

5.2 Void 20

5.3 Void 20

5.4 Void 20

5.5 Operating bands 20

5.5A Operating bands for CA 22

5.5B Operating bands for UL-MIMO 22

5.6 Channel bandwidth 22

5.6.1 Channel bandwidths per operating band 23

5.6A Channel bandwidth for CA 24

5.6A.1 Channel bandwidths per operating band for CA 26

5.6B Channel bandwidth for UL-MIMO 27

5.6B.1 Void 27

5.7 Channel arrangement 27

5.7.1 Channel spacing 27

5.7.1A Channel spacing for CA 27

5.7.2 Channel raster 27

5.7.2A Channel raster for CA 28

5.7.3 Carrier frequency and EARFCN 28

5.7.4 TX–RX frequency separation 29

5.7.4A TX–RX frequency separation for CA 30

6 Transmitter characteristics 30

6.1 General 30

6.2 Transmit power 30

6.2.1 Void 30

6.2.2 UE maximum output power 30

6.2.2A UE maximum output power for CA 31

6.2.2B UE maximum output power for UL-MIMO 32

6.2.3 UE maximum output power for modulation / channel bandwidth 33

6.2.3A UE Maximum Output power for modulation / channel bandwidth for CA 34

6.2.3B UE maximum output power for modulation / channel bandwidth for UL-MIMO 35

6.2.4 UE maximum output power with additional requirements 35

6.2.4A UE maximum output power with additional requirements for CA 41

6.2.4A.1 A-MPR for CA\_NS\_01 for CA\_1C 42

6.2.4A.2 A-MPR for CA\_NS\_02 for CA\_1C 43

6.2.4A.3 A-MPR for CA\_NS\_03 for CA\_1C 43

6.2.4B UE maximum output power with additional requirements for UL-MIMO 44

6.2.5 Configured transmitted power 44

6.2.5A Configured transmitted power for CA 46

6.2.5B Configured transmitted power for UL-MIMO 47

6.3 Output power dynamics 48

6.3.1 (Void) 48

6.3.2 Minimum output power 48

6.3.2.1 Minimum requirement 48

6.3.2A UE Minimum output power for CA 48

6.3.2A.1 Minimum requirement for CA 48

6.3.2B UE Minimum output power for UL-MIMO 49

6.3.2B.1 Minimum requirement 49

6.3.3 Transmit OFF power 49

6.3.3.1. Minimum requirement 49

6.3.3A UE Transmit OFF power for CA 50

6.3.3A.1 Minimum requirement for CA 50

6.3.3B UE Transmit OFF power for UL-MIMO 50

6.3.3B.1 Minimum requirement 50

6.3.4 ON/OFF time mask 50

6.3.4.1 General ON/OFF time mask 50

6.3.4.2 PRACH and SRS time mask 51

6.3.4.2.1 PRACH time mask 51

6.3.4.2.2 SRS time mask 51

6.3.4.3 Slot / Sub frame boundary time mask 52

6.3.4.4 PUCCH / PUSCH / SRS time mask 53

6.3.4A ON/OFF time mask for CA 54

6.3.4B ON/OFF time mask for UL-MIMO 54

6.3.5 Power Control 54

6.3.5.1 Absolute power tolerance 54

6.3.5.1.1 Minimum requirements 55

6.3.5.2 Relative Power tolerance 55

6.3.5.2.1 Minimum requirements 55

6.3.5.3 Aggregate power control tolerance 56

6.3.5.3.1 Minimum requirement 56

6.3.5A Power control for CA 57

6.3.5A.1 Absolute power tolerance 57

6.3.5A.1.1 Minimum requirements 57

6.3.5A.2 Relative power tolerance 57

6.3.5A.2.1 Minimum requirements 57

6.3.5A.3 Aggregate power control tolerance 57

6.3.5A.3.1 Minimum requirements 58

6.3.5B Power control for UL-MIMO 58

6.4 Void 58

6.5 Transmit signal quality 58

6.5.1 Frequency error 58

6.5.1A Frequency error for CA 58

6.5.1B Frequency error for UL-MIMO 58

6.5.2 Transmit modulation quality 58

6.5.2.1 Error Vector Magnitude 59

6.5.2.1.1 Minimum requirement 59

6.5.2.2 Carrier leakage 59

6.5.2.2.1 Minimum requirements 59

6.5.2.3 In-band emissions 60

6.5.2.3.1 Minimum requirements 60

6.5.2.4 EVM equalizer spectrum flatness 60

6.5.2.4.1 Minimum requirements 61

6.5.2A Transmit modulation quality for CA 62

6.5.2A.1 Error Vector Magnitude 62

6.5.2A.2 Carrier leakage for CA 62

6.5.2A.2.1 Minimum requirements 62

6.5.2A.3 In-band emissions 62

6.5.2A.3.1 Minimum requirement for CA 62

6.5.2B Transmit modulation quality for UL-MIMO 64

6.5.2B.1 Error Vector Magnitude 65

6.5.2B.2 Carrier leakage 65

6.5.2B.3 In-band emissions 65

6.5.2B.4 EVM equalizer spectrum flatness for UL-MIMO 65

6.6 Output RF spectrum emissions 65

6.6.1 Occupied bandwidth 66

6.6.1A Occupied bandwidth for CA 66

6.6.1B Occupied bandwidth for UL-MIMO 66

6.6.2 Out of band emission 66

6.6.2.1 Spectrum emission mask 66

6.6.2.1.1 Minimum requirement 67

6.6.2.1A Spectrum emission mask for CA 67

6.6.2.2 Additional spectrum emission mask 67

6.6.2.2.1 Minimum requirement (network signalled value "NS\_03", “NS\_11”, and “NS\_20”) 67

6.6.2.2.2 Minimum requirement (network signalled value "NS\_04") 68

6.6.2.2.3 Minimum requirement (network signalled value "NS\_06" or “NS\_07”) 68

6.6.2.3 Adjacent Channel Leakage Ratio 69

6.6.2.3.1 Minimum requirement E-UTRA 69

6.6.2.3.1A Void 70

6.6.2.3.2 Minimum requirements UTRA 70

6.6.2.3.2A Minimum requirement UTRA for CA 71

6.6.2.3.3A Minimum requirements for CA E-UTRA 71

6.6.2.4 Void 72

6.6.2.4.1 Void 72

6.6.2A Void 72

6.6.2B Out of band emission for UL-MIMO 72

6.6.3 Spurious emissions 72

6.6.3.1 Minimum requirements 72

6.6.3.1A Minimum requirements for CA 73

6.6.3.2 Spurious emission band UE co-existence 73

6.6.3.2A Spurious emission band UE co-existence for CA 77

6.6.3.3 Additional spurious emissions 78

6.6.3.3.1 Minimum requirement (network signalled value "NS\_05") 78

6.6.3.3.2 Minimum requirement (network signalled value “NS\_07”) 79

6.6.3.3.3 Minimum requirement (network signalled value “NS\_08”) 79

6.6.3.3.4 Minimum requirement (network signalled value “NS\_09”) 79

6.6.3.3.5 Void 80

6.6.3.3.6 Void 80

6.6.3.3.7 Void 80

6.6.3.3.8 Void 80

6.6.3.3.9 Void 80

6.6.3.3.10 Void 80

6.6.3.3.11 Void 80

6.6.3.3.12 Void 80

6.6.3.3.13 Minimum requirement (network signalled value " NS\_11") 80

6.6.3.3.14 Minimum requirement (network signalled value " NS\_20") 80

6.6.3.3.15 Minimum requirement (network signalled value "NS\_22") 81

6.6.3.3.16 Minimum requirement (network signalled value "NS\_23") 81

6.6.3.3.17 Void 82

6.6.3.3.18 Void 82

6.6.3.3.19 Void 82

6.6.3.3.20 Void 83

6.6.3.3.21 Void 83

6.6.3.3.22 Void 83

6.6.3.3.23 Void 83

6.6.3.3.24 Void 83

6.6.3.3.25 Void 83

6.6.3.3.26 Void 83

6.6.3.3.27 Void 83

6.6.3.3.28 Void 83

6.6.3.3.29 Void 83

6.6.3.3.30 Void 84

6.6.3.3.31 Void 84

6.6.3.3.32 Void 84

6.6.3.3.33 Void 84

6.6.3.3.34 Void 84

6.6.3.3.35 Minimum requirement (network signalled value “NS\_56”) 84

6.6.3.3A Additional spurious emissions for CA 84

6.6.3.3A.1 Minimum requirement for CA\_1C (network signalled value "CA\_NS\_01") 85

6.6.3.3A.2 Minimum requirement for CA\_1C (network signalled value "CA\_NS\_02") 85

6.6.3.3A.3 Minimum requirement for CA\_1C (network signalled value "CA\_NS\_03") 85

6.6.3A Void 85

6.6.3B Spurious emission for UL-MIMO 86

6.6A Void 86

6.6B Void 86

6.7 Transmit intermodulation 86

6.7.1 Minimum requirement 86

6.7.1A Minimum requirement for CA 86

6.7.1B Minimum requirement for UL-MIMO 87

6.8 Void 87

6.8.1 Void 87

6.8A Void 87

6.8B Time alignment error for UL-MIMO 87

6.8B.1 Minimum Requirements 87

7 Receiver characteristics 87

7.1 General 87

7.2 Diversity characteristics 88

7.3 Reference sensitivity power level 88

7.3.1 Minimum requirements (QPSK) 88

7.3.1A Minimum requirements (QPSK) for CA 92

7.3.1B Minimum requirements (QPSK) for UL-MIMO 93

7.3.2 Void 93

7.4 Maximum input level 93

7.4.1 Minimum requirements 93

7.4.1A Minimum requirements for CA 93

7.4.1B Minimum requirements for UL-MIMO 94

7.4A Void 94

7.4A.1 Void 94

7.5 Adjacent Channel Selectivity (ACS) 94

7.5.1 Minimum requirements 94

7.5.1A Minimum requirements for CA 95

7.5.1B Minimum requirements for UL-MIMO 96

7.6 Blocking characteristics 96

7.6.1 In-band blocking 97

7.6.1.1 Minimum requirements 97

7.6.1.1A Minimum requirements for CA 97

7.6.2 Out-of-band blocking 98

7.6.2.1 Minimum requirements 99

7.6.2.1A Minimum requirements for CA 99

7.6.3 Narrow band blocking 101

7.6.3.1 Minimum requirements 101

7.6.3.1A Minimum requirements for CA 101

7.6A Void 102

7.6B Blocking characteristics for UL-MIMO 102

7.7 Spurious response 102

7.7.1 Minimum requirements 102

7.7.1A Minimum requirements for CA 103

7.7.1B Minimum requirements for UL-MIMO 103

7.8 Intermodulation characteristics 103

7.8.1 Wide band intermodulation 104

7.8.1.1 Minimum requirements 104

7.8.1A Minimum requirements for CA 104

7.8.1B Minimum requirements for UL-MIMO 105

7.8.2 Void 105

7.9 Spurious emissions 105

7.9.1 Minimum requirements 106

7.10 Receiver image 106

7.10.1 Void 106

7.10.1A Minimum requirements for CA 106

8 Performance requirement 107

8.1 General 107

8.1.1 Dual-antenna receiver capability 107

8.1.1.1 Simultaneous unicast and MBMS operations 107

8.1.1.2 Dual-antenna receiver capability in idle mode 107

8.1.2 Applicability of requirements 107

8.1.2.1 Applicability of requirements for different channel bandwidths 107

8.1.2.2 Definition of CA capability 107

8.1.2.3 Applicability and test rules for different CA configurations and bandwidth combination sets 108

8.1.2.4 Test coverage for different number of component carriers 109

8.2 Demodulation of PDSCH (Cell-Specific Reference Symbols) 110

8.2.1 FDD (Fixed Reference Channel) 110

8.2.1.1 Single-antenna port performance 110

8.2.1.1.1 Minimum Requirement 110

8.2.1.1.2 Void 113

8.2.1.1.3 Void 113

8.2.1.1.4 Minimum Requirement 1 PRB allocation in presence of MBSFN 113

8.2.1.2 Transmit diversity performance 114

8.2.1.2.1 Minimum Requirement 2 Tx Antenna Port 114

8.2.1.2.2 Minimum Requirement 4 Tx Antenna Port 114

8.2.1.2.3 Minimum Requirement 2 Tx Antenna Ports (demodulation subframe overlaps with aggressor cell ABS) 115

8.2.1.3 Open-loop spatial multiplexing performance 117

8.2.1.3.1 Minimum Requirement 2 Tx Antenna Port 117

8.2.1.3.1A Soft buffer management test 118

8.2.1.3.2 Minimum Requirement 4 Tx Antenna Port 119

8.2.1.3.3 Minimum Requirement 2 Tx Antenna Port (demodulation subframe overlaps with aggressor cell ABS) 119

8.2.1.4 Closed-loop spatial multiplexing performance 123

8.2.1.4.1 Minimum Requirement Single-Layer Spatial Multiplexing 2 Tx Antenna Port 123

8.2.1.4.1A Minimum Requirement Single-Layer Spatial Multiplexing 4 Tx Antenna Port 124

8.2.1.4.2 Minimum Requirement Multi-Layer Spatial Multiplexing 2 Tx Antenna Port 124

8.2.1.4.3 Minimum Requirement Multi-Layer Spatial Multiplexing 4 Tx Antenna Port 125

8.2.1.5 MU-MIMO 127

8.2.1.6 [Control channel performance: D-BCH and PCH] 127

8.2.1.7 Carrier aggregation with power imbalance 127

8.2.1.7.1 Minimum Requirement 127

8.2.2 TDD (Fixed Reference Channel) 128

8.2.2.1 Single-antenna port performance 129

8.2.2.1.1 Minimum Requirement 129

8.2.2.1.2 Void 132

8.2.2.1.3 Void 132

8.2.2.1.4 Minimum Requirement 1 PRB allocation in presence of MBSFN 132

8.2.2.2 Transmit diversity performance 132

8.2.2.2.1 Minimum Requirement 2 Tx Antenna Port 132

8.2.2.2.2 Minimum Requirement 4 Tx Antenna Port 133

8.2.2.2.3 Minimum Requirement 2 Tx Antenna Port (demodulation subframe overlaps with aggressor cell ABS) 134

8.2.2.3 Open-loop spatial multiplexing performance 135

8.2.2.3.1 Minimum Requirement 2 Tx Antenna Port 135

8.2.2.3.1A Soft buffer management test 136

8.2.2.3.2 Minimum Requirement 4 Tx Antenna Port 137

8.2.2.3.3 Minimum Requirement 2Tx antenna port (demodulation subframe overlaps with aggressor cell ABS) 137

8.2.2.4 Closed-loop spatial multiplexing performance 141

8.2.2.4.1 Minimum Requirement Single-Layer Spatial Multiplexing 2 Tx Antenna Port 141

8.2.2.4.1A Minimum Requirement Single-Layer Spatial Multiplexing 4 Tx Antenna Port 142

8.2.2.4.2 Minimum Requirement Multi-Layer Spatial Multiplexing 2 Tx Antenna Port 142

8.2.2.4.3 Minimum Requirement Multi-Layer Spatial Multiplexing 4 Tx Antenna Port 143

8.2.2.5 MU-MIMO 145

8.2.2.6 [Control channel performance: D-BCH and PCH] 145

8.2.2.7 Carrier aggregation with power imbalance 145

8.2.2.7.1 Minimum Requirement 145

8.3 Demodulation of PDSCH (User-Specific Reference Symbols) 146

8.3.1 FDD 146

8.3.1.1 Single-layer Spatial Multiplexing 147

8.3.1.2 Dual-Layer Spatial Multiplexing 149

8.3.2 TDD 150

8.3.2.1 Single-layer Spatial Multiplexing 150

8.3.2.1A Single-layer Spatial Multiplexing (with multiple CSI-RS configurations) 153

8.3.2.2 Dual-Layer Spatial Multiplexing 154

8.3.2.3 Dual-Layer Spatial Multiplexing (with multiple CSI-RS configurations) 155

8.4 Demodulation of PDCCH/PCFICH 156

8.4.1 FDD 156

8.4.1.1 Single-antenna port performance 156

8.4.1.2 Transmit diversity performance 157

8.4.1.2.1 Minimum Requirement 2 Tx Antenna Port 157

8.4.1.2.2 Minimum Requirement 4 Tx Antenna Port 157

8.4.1.2.3 Minimum Requirement 2 Tx Antenna Port (demodulation subframe overlaps with aggressor cell ABS) 157

8.4.2 TDD 162

8.4.2.1 Single-antenna port performance 163

8.4.2.2 Transmit diversity performance 163

8.4.2.2.1 Minimum Requirement 2 Tx Antenna Port 163

8.4.2.2.2 Minimum Requirement 4 Tx Antenna Port 164

8.4.2.2.3 Minimum Requirement 2 Tx Antenna Port (demodulation subframe overlaps with aggressor cell ABS) 164

8.5 Demodulation of PHICH 168

8.5.1 FDD 168

8.5.1.1 Single-antenna port performance 168

8.5.1.2 Transmit diversity performance 169

8.5.1.2.1 Minimum Requirement 2 Tx Antenna Port 169

8.5.1.2.2 Minimum Requirement 4 Tx Antenna Port 169

8.5.1.2.3 Minimum Requirement 2 Tx Antenna Port (demodulation subframe overlaps with aggressor cell ABS) 169

8.5.2 TDD 171

8.5.2.1 Single-antenna port performance 171

8.5.2.2 Transmit diversity performance 172

8.5.2.2.1 Minimum Requirement 2 Tx Antenna Port 172

8.5.2.2.2 Minimum Requirement 4 Tx Antenna Port 172

8.5.2.2.3 Minimum Requirement 2 Tx Antenna Port (demodulation subframe overlaps with aggressor cell ABS) 172

8.6 Demodulation of PBCH 174

8.6.1 FDD 174

8.6.1.1 Single-antenna port performance 174

8.6.1.2 Transmit diversity performance 174

8.6.1.2.1 Minimum Requirement 2 Tx Antenna Port 174

8.6.1.2.2 Minimum Requirement 4 Tx Antenna Port 175

8.6.2 TDD 175

8.6.2.1 Single-antenna port performance 175

8.6.2.2 Transmit diversity performance 176

8.6.2.2.1 Minimum Requirement 2 Tx Antenna Port 176

8.6.2.2.2 Minimum Requirement 4 Tx Antenna Port 176

8.7 Sustained downlink data rate provided by lower layers 176

8.7.1 FDD 176

8.7.2 TDD 178

9 Reporting of Channel State Information 180

9.1 General 180

9.1.1 Applicability of requirements 180

9.1.1.1 Applicability of requirements for different channel bandwidths 180

9.1.1.2 Applicability and test rules for different CA configurations and bandwidth combination sets 181

9.2 CQI reporting definition under AWGN conditions 181

9.2.1 Minimum requirement PUCCH 1-0 (Cell-Specific Reference Symbols) 181

9.2.1.1 FDD 181

9.2.1.2 TDD 182

9.2.1.3 FDD (CSI measurements in case two CSI subframe sets are configured) 183

9.2.1.4 TDD (CSI measurements in case two CSI subframe sets are configured) 186

9.2.2 Minimum requirement PUCCH 1-1 (Cell-Specific Reference Symbols) 189

9.2.2.1 FDD 189

9.2.2.2 TDD 190

9.2.3 Minimum requirement PUCCH 1-1 (CSI Reference Symbols) 191

9.2.3.1 FDD 191

9.2.3.2 TDD 192

9.3 CQI reporting under fading conditions 193

9.3.1 Frequency-selective scheduling mode 193

9.3.1.1 Minimum requirement PUSCH 3-0 (Cell-Specific Reference Symbols) 194

9.3.1.1.1 FDD 194

9.3.1.1.2 TDD 195

9.3.1.2 Minimum requirement PUSCH 3-1 (CSI Reference Symbol) 196

9.3.1.2.1 FDD 196

9.3.1.2.2 TDD 197

9.3.2 Frequency non-selective scheduling mode 199

9.3.2.1 Minimum requirement PUCCH 1-0 (Cell-Specific Reference Symbol) 199

9.3.2.1.1 FDD 199

9.3.2.1.2 TDD 200

9.3.2.2 Minimum requirement PUCCH 1-1 (CSI Reference Symbol) 202

9.3.2.2.1 FDD 202

9.3.2.2.2 TDD 203

9.3.3 Frequency-selective interference 205

9.3.3.1 Minimum requirement PUSCH 3-0 (Cell-Specific Reference Symbol) 205

9.3.3.1.1 FDD 205

9.3.3.1.2 TDD 206

9.3.3.2 Void 207

9.3.3.2.1 Void 207

9.3.3.2.2 Void 207

9.3.4 UE-selected subband CQI 207

9.3.4.1 Minimum requirement PUSCH 2-0 (Cell-Specific Reference Symbols) 207

9.3.4.1.1 FDD 207

9.3.4.1.2 TDD 208

9.3.4.2 Minimum requirement PUCCH 2-0 (Cell-Specific Reference Symbols) 209

9.3.4.2.1 FDD 209

9.3.4.2.2 TDD 211

9.4 Reporting of Precoding Matrix Indicator (PMI) 213

9.4.1 Single PMI 213

9.4.1.1 Minimum requirement PUSCH 3-1 (Cell-Specific Reference Symbols) 213

9.4.1.1.1 FDD 213

9.4.1.1.2 TDD 214

9.4.1.2 Minimum requirement PUCCH 2-1 (Cell-Specific Reference Symbols) 215

9.4.1.2.1 FDD 215

9.4.1.2.2 TDD 217

9.4.1.3 Minimum requirement PUSCH 3-1 (CSI Reference Symbol) 219

9.4.1.3.1 FDD 219

9.4.1.3.2 TDD 220

9.4.1a Void 223

9.4.1a.1 Void 223

9.4.1a.1.1 Void 223

9.4.1a.1.2 Void 223

9.4.2 Multiple PMI 223

9.4.2.1 Minimum requirement PUSCH 1-2 (Cell-Specific Reference Symbols) 223

9.4.2.1.1 FDD 223

9.4.2.1.2 TDD 224

9.4.2.2 Minimum requirement PUSCH 2-2 (Cell-Specific Reference Symbols) 225

9.4.2.2.1 FDD 225

9.4.2.2.2 TDD 226

9.4.2.3 Minimum requirement PUSCH 1-2 (CSI Reference Symbol) 227

9.4.2.3.1 FDD 227

9.4.2.3.2 TDD 229

9.4.3 Void 232

9.4.3.1 Void 232

9.4.3.1.1 Void 232

9.4.3.1.2 Void 232

9.5 Reporting of Rank Indicator (RI) 232

9.5.1 Minimum requirement (Cell-Specific Reference Symbols) 232

9.5.1.1 FDD 232

9.5.1.2 TDD 234

9.5.2 Minimum requirement (CSI Reference Symbols) 235

9.5.2.1 FDD 235

9.5.2.2 TDD 237

9.5.3 Minimum requirement (CSI measurements in case two CSI subframe sets are configured) 239

9.5.3.1 FDD 239

9.5.3.2 TDD 242

9.6 Additional requirements for carrier aggregation 245

9.6.1 Periodic reporting on multiple cells (Cell-Specific Reference Symbols) 245

9.6.1.1 FDD 245

9.6.1.2 TDD 246

10 Performance requirement (MBMS) 247

10.1 FDD (Fixed Reference Channel) 247

10.1.1 Minimum requirement 248

10.2 TDD (Fixed Reference Channel) 248

10.2.1 Minimum requirement 249

Annex A (normative): Measurement channels 250

A.1 General 250

A.2 UL reference measurement channels 250

A.2.1 General 250

A.2.1.1 Applicability and common parameters 250

A.2.1.2 Determination of payload size 250

A.2.1.3 Overview of UL reference measurement channels 251

A.2.2 Reference measurement channels for FDD 256

A.2.2.1 Full RB allocation 256

A.2.2.1.1 QPSK 256

A.2.2.1.2 16-QAM 257

A.2.2.1.3 64-QAM 257

A.2.2.2 Partial RB allocation 257

A.2.2.2.1 QPSK 258

A.2.2.2.2 16-QAM 259

A.2.2.2.3 64-QAM 259

A.2.2.3 Void 259

A.2.3 Reference measurement channels for TDD 259

A.2.3.1 Full RB allocation 260

A.2.3.1.1 QPSK 260

A.2.3.1.2 16-QAM 260

A.2.3.1.3 64-QAM 260

A.2.3.2 Partial RB allocation 261

A.2.3.2.1 QPSK 261

A.2.3.2.2 16-QAM 262

A.2.3.2.3 64-QAM 262

A.2.3.3 Void 263

A.3 DL reference measurement channels 263

A.3.1 General 263

A.3.1.1 Overview of DL reference measurement channels 263

A.3.2 Reference measurement channel for receiver characteristics 269

A.3.3 Reference measurement channels for PDSCH performance requirements (FDD) 277

A.3.3.1 Single-antenna transmission (Common Reference Symbols) 277

A.3.3.2 Multi-antenna transmission (Common Reference Symbols) 283

A.3.3.2.1 Two antenna ports 283

A.3.3.2.2 Four antenna ports 284

A.3.3.3 Reference Measurement Channel for UE-Specific Reference Symbols 284

A.3.3.3.1 Two antenna port (CSI-RS) 284

A.3.3.3.2 Four antenna ports (CSI-RS) 285

A.3.4 Reference measurement channels for PDSCH performance requirements (TDD) 288

A.3.4.1 Single-antenna transmission (Common Reference Symbols) 288

A.3.4.2 Multi-antenna transmission (Common Reference Signals) 296

A.3.4.2.1 Two antenna ports 296

A.3.4.2.2 Four antenna ports 297

A.3.4.3 Reference Measurement Channels for UE-Specific Reference Symbols 297

A.3.4.3.1 Single antenna port (Cell Specific) 297

A.3.4.3.2 Two antenna ports (Cell Specific) 298

A.3.4.3.3 Two antenna ports (CSI-RS) 299

A.3.4.3.4 Four antenna ports (CSI-RS) 300

A.3.4.3.5 Eight antenna ports (CSI-RS) 301

A.3.5 Reference measurement channels for PDCCH/PCFICH performance requirements 304

A.3.5.1 FDD 304

A.3.5.2 TDD 304

A.3.6 Reference measurement channels for PHICH performance requirements 304

A.3.7 Reference measurement channels for PBCH performance requirements 305

A.3.8 Reference measurement channels for MBMS performance requirements 305

A.3.8.1 FDD 305

A.3.8.2 TDD 307

A.3.9 Reference measurement channels for sustained downlink data rate provided by lower layers 309

A.3.9.1 FDD 309

A.3.9.2 TDD 310

A.4 CSI reference measurement channels 311

A.5 OFDMA Channel Noise Generator (OCNG) 314

A.5.1 OCNG Patterns for FDD 314

A.5.1.1 OCNG FDD pattern 1: One sided dynamic OCNG FDD pattern 315

A.5.1.2 OCNG FDD pattern 2: Two sided dynamic OCNG FDD pattern 315

A.5.1.3 OCNG FDD pattern 3: 49 RB OCNG allocation with MBSFN in 10 MHz 316

A.5.1.4 OCNG FDD pattern 4: One sided dynamic OCNG FDD pattern for MBMS transmission 317

A.5.1.5 OCNG FDD pattern 5: One sided dynamic 16QAM modulated OCNG FDD pattern 317

A.5.1.6 OCNG FDD pattern 6: dynamic OCNG FDD pattern when user data is in 2 non-contiguous blocks 318

A.5.2 OCNG Patterns for TDD 319

A.5.2.1 OCNG TDD pattern 1: One sided dynamic OCNG TDD pattern 320

A.5.2.2 OCNG TDD pattern 2: Two sided dynamic OCNG TDD pattern 320

A.5.2.3 OCNG TDD pattern 3: 49 RB OCNG allocation with MBSFN in 10 MHz 321

A.5.2.4 OCNG TDD pattern 4: One sided dynamic OCNG TDD pattern for MBMS transmission 322

A.5.2.5 OCNG TDD pattern 5: One sided dynamic 16QAM modulated OCNG TDD pattern 322

A.5.2.6 OCNG TDD pattern 6: dynamic OCNG TDD pattern when user data is in 2 non-contiguous blocks 323

Annex B (normative): Propagation conditions 325

B.1 Static propagation condition 325

B.2 Multi-path fading propagation conditions 325

B.2.1 Delay profiles 325

B.2.2 Combinations of channel model parameters 326

B.2.3 MIMO Channel Correlation Matrices 327

B.2.3.1 Definition of MIMO Correlation Matrices 327

B.2.3.2 MIMO Correlation Matrices at High, Medium and Low Level 328

B.2.3A MIMO Channel Correlation Matrices using cross polarized antennas 330

B.2.3A.1 Definition of MIMO Correlation Matrices using cross polarized antennas 331

B.2.3A.2 Spatial Correlation Matrices using cross polarized antennas at eNB and UE sides 331

B.2.3A.2.1 Spatial Correlation Matrices at eNB side 331

B.2.3A.2.2 Spatial Correlation Matrices at UE side 331

B.2.3A.4 Beam steering approach 332

B.2.4 Propagation conditions for CQI tests 333

B.2.5 Void 333

B.2.6 MBSFN Propagation Channel Profile 333

B.3 High speed train scenario 334

B.4 Beamforming Model 335

B.4.1 Single-layer random beamforming (Antenna port 5, 7, or 8) 335

B.4.2 Dual-layer random beamforming (antenna ports 7 and 8) 336

B.4.3 Generic beamforming model (antenna ports 7-14) 336

Annex C (normative): Downlink Physical Channels 338

C.1 General 338

C.2 Set-up 338

C.3 Connection 338

C.3.1 Measurement of Receiver Characteristics 338

C.3.2 Measurement of Performance requirements 339

C.3.3 Aggressor cell power allocation for Measurement of Performance Requirements when ABS is Configured 340

Annex D (normative): Characteristics of the interfering signal 341

D.1 General 341

D.2 Interference signals 341

Annex E (normative): Environmental conditions 342

E.1 General 342

E.2 Environmental 342

E.2.1 Temperature 342

E.2.2 Voltage 342

E.2.3 Vibration 343

Annex F (normative): Transmit modulation 344

F.1 Measurement Point 344

F.2 Basic Error Vector Magnitude measurement 344

F.3 Basic in-band emissions measurement 345

F.4 Modified signal under test 345

F.5 Window length 347

F.5.1 Timing offset 347

F.5.2 Window length 347

F.5.3 Window length for normal CP 347

F.5.4 Window length for Extended CP 348

F.5.5 Window length for PRACH 348

F.6 Averaged EVM 349

F.7 Spectrum Flatness 350

Annex G (informative): Reference sensitivity level in lower SNR 351

G.1 General 351

G.2 Typical receiver sensitivity performance (QPSK) 351

G.3 Reference measurement channel for REFSENSE in lower SNR 354

Annex H (normative): Modified MPR behavior 356

H.1 Indication of modified MPR behavior 356

Annex I (informative): Change history 358