3GPP TS 36.101 V11.30.0 (2022-09)

Technical Specification

3rd Generation Partnership Project;

Technical Specification Group Radio Access Network;

Evolved Universal Terrestrial Radio Access (E-UTRA);

User Equipment (UE) radio transmission and reception

(Release 11)

 

The present document has been developed within the 3rd Generation Partnership Project (3GPP TM) and may be further elaborated for the purposes of 3GPP.  
The present document has not been subject to any approval process by the 3GPPOrganizational Partners and shall not be implemented.  
This Specification is provided for future development work within 3GPPonly. The Organizational Partners accept no liability for any use of this Specification.  
Specifications and reports for implementation of the 3GPP TM system should be obtained via the 3GPP Organizational Partners' Publications Offices.

***3GPP***

Postal address

3GPP support office address

650 Route des Lucioles - Sophia Antipolis

Valbonne - FRANCE

Tel.: +33 4 92 94 42 00 Fax: +33 4 93 65 47 16

Internet

http://www.3gpp.org

***Copyright Notification***

No part may be reproduced except as authorized by written permission.  
The copyright and the foregoing restriction extend to reproduction in all media.

© 2022, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

All rights reserved.

UMTS™ is a Trade Mark of ETSI registered for the benefit of its members

3GPP™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners  
LTE™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners

GSM® and the GSM logo are registered and owned by the GSM Association

Contents

Foreword 16

1 Scope 17

2 References 17

3 Definitions, symbols and abbreviations 17

3.1 Definitions 17

3.2 Symbols 18

3.3 Abbreviations 21

4 General 22

4.1 Relationship between minimum requirements and test requirements 22

4.2 Applicability of minimum requirements 22

4.3 Void 22

4.3A Applicability of minimum requirements (CA, UL-MIMO) 22

4.4 RF requirements in later releases 23

5 Operating bands and channel arrangement 23

5.1 General 23

5.2 Void 23

5.3 Void 23

5.4 Void 23

5.5 Operating bands 23

5.5A Operating bands for CA 26

5.5B Operating bands for UL-MIMO 28

5.6 Channel bandwidth 28

5.6.1 Channel bandwidths per operating band 29

5.6A Channel bandwidth for CA 30

5.6A.1 Channel bandwidths per operating band for CA 32

5.6B Channel bandwidth for UL-MIMO 35

5.6B.1 Void 35

5.7 Channel arrangement 35

5.7.1 Channel spacing 35

5.7.1A Channel spacing for CA 35

5.7.2 Channel raster 35

5.7.2A Channel raster for CA 36

5.7.3 Carrier frequency and EARFCN 36

5.7.4 TX–RX frequency separation 37

5.7.4A TX–RX frequency separation for CA 38

6 Transmitter characteristics 38

6.1 General 38

6.2 Transmit power 38

6.2.1 Void 38

6.2.2 UE maximum output power 38

6.2.2A UE maximum output power for CA 39

6.2.2B UE maximum output power for UL-MIMO 40

6.2.3 UE maximum output power for modulation / channel bandwidth 42

6.2.3A UE Maximum Output power for modulation / channel bandwidth for CA 42

6.2.3B UE maximum output power for modulation / channel bandwidth for UL-MIMO 43

6.2.4 UE maximum output power with additional requirements 43

6.2.4A UE maximum output power with additional requirements for CA 52

6.2.4A.1 A-MPR for CA\_NS\_01 for CA\_1C 53

6.2.4A.2 A-MPR for CA\_NS\_02 for CA\_1C 54

6.2.4A.3 A-MPR for CA\_NS\_03 for CA\_1C 54

6.2.4A.4 A-MPR for CA\_NS\_04 55

6.2.4A.5 A-MPR for CA\_NS\_05 for CA\_38C 56

6.2.4A.6 A-MPR for CA\_NS\_06 56

6.2.4B UE maximum output power with additional requirements for UL-MIMO 57

6.2.5 Configured transmitted power 57

6.2.5A Configured transmitted power for CA 60

6.2.5B Configured transmitted power for UL-MIMO 61

6.3 Output power dynamics 62

6.3.1 (Void) 62

6.3.2 Minimum output power 62

6.3.2.1 Minimum requirement 62

6.3.2A UE Minimum output power for CA 62

6.3.2A.1 Minimum requirement for CA 62

6.3.2B UE Minimum output power for UL-MIMO 62

6.3.2B.1 Minimum requirement 63

6.3.3 Transmit OFF power 63

6.3.3.1. Minimum requirement 63

6.3.3A UE Transmit OFF power for CA 63

6.3.3A.1 Minimum requirement for CA 63

6.3.3B UE Transmit OFF power for UL-MIMO 64

6.3.3B.1 Minimum requirement 64

6.3.4 ON/OFF time mask 64

6.3.4.1 General ON/OFF time mask 64

6.3.4.2 PRACH and SRS time mask 65

6.3.4.2.1 PRACH time mask 65

6.3.4.2.2 SRS time mask 65

6.3.4.3 Slot / Sub frame boundary time mask 66

6.3.4.4 PUCCH / PUSCH / SRS time mask 66

6.3.4A ON/OFF time mask for CA 68

6.3.4B ON/OFF time mask for UL-MIMO 68

6.3.5 Power Control 68

6.3.5.1 Absolute power tolerance 68

6.3.5.1.1 Minimum requirements 68

6.3.5.2 Relative Power tolerance 69

6.3.5.2.1 Minimum requirements 69

6.3.5.3 Aggregate power control tolerance 70

6.3.5.3.1 Minimum requirement 70

6.3.5A Power control for CA 70

6.3.5A.1 Absolute power tolerance 70

6.3.5A.1.1 Minimum requirements 70

6.3.5A.2 Relative power tolerance 70

6.3.5A.2.1 Minimum requirements 70

6.3.5A.3 Aggregate power control tolerance 71

6.3.5A.3.1 Minimum requirements 71

6.3.5B Power control for UL-MIMO 71

6.4 Void 71

6.5 Transmit signal quality 71

6.5.1 Frequency error 71

6.5.1A Frequency error for CA 72

6.5.1B Frequency error for UL-MIMO 72

6.5.2 Transmit modulation quality 72

6.5.2.1 Error Vector Magnitude 72

6.5.2.1.1 Minimum requirement 72

6.5.2.2 Carrier leakage 73

6.5.2.2.1 Minimum requirements 73

6.5.2.3 In-band emissions 73

6.5.2.3.1 Minimum requirements 73

6.5.2.4 EVM equalizer spectrum flatness 74

6.5.2.4.1 Minimum requirements 74

6.5.2A Transmit modulation quality for CA 75

6.5.2A.1 Error Vector Magnitude 75

6.5.2A.2 Carrier leakage for CA 76

6.5.2A.2.1 Minimum requirements 76

6.5.2A.3 In-band emissions 76

6.5.2A.3.1 Minimum requirement for CA 76

6.5.2B Transmit modulation quality for UL-MIMO 78

6.5.2B.1 Error Vector Magnitude 79

6.5.2B.2 Carrier leakage 79

6.5.2B.3 In-band emissions 79

6.5.2B.4 EVM equalizer spectrum flatness for UL-MIMO 79

6.6 Output RF spectrum emissions 79

6.6.1 Occupied bandwidth 80

6.6.1A Occupied bandwidth for CA 80

6.6.1B Occupied bandwidth for UL-MIMO 80

6.6.2 Out of band emission 80

6.6.2.1 Spectrum emission mask 80

6.6.2.1.1 Minimum requirement 80

6.6.2.1A Spectrum emission mask for CA 81

6.6.2.2 Additional spectrum emission mask 81

6.6.2.2.1 Minimum requirement (network signalled value "NS\_03", “NS\_11”, and “NS\_20”) 81

6.6.2.2.2 Minimum requirement (network signalled value "NS\_04") 82

6.6.2.2.3 Minimum requirement (network signalled value "NS\_06" or “NS\_07”) 82

6.6.2.2A Additional Spectrum Emission Mask for CA 83

6.6.2.2A.1 Minimum requirement (network signalled value "CA\_NS\_04") 83

6.6.2.3 Adjacent Channel Leakage Ratio 83

6.6.2.3.1 Minimum requirement E-UTRA 84

6.6.2.3.1A Void 84

6.6.2.3.2 Minimum requirements UTRA 84

6.6.2.3.2A Minimum requirement UTRA for CA 85

6.6.2.3.3A Minimum requirements for CA E-UTRA 86

6.6.2.4 Void 86

6.6.2.4.1 Void 86

6.6.2A Void 86

6.6.2B Out of band emission for UL-MIMO 86

6.6.3 Spurious emissions 87

6.6.3.1 Minimum requirements 87

6.6.3.1A Minimum requirements for CA 87

6.6.3.2 Spurious emission band UE co-existence 88

6.6.3.2A Spurious emission band UE co-existence for CA 94

6.6.3.3 Additional spurious emissions 95

6.6.3.3.1 Minimum requirement (network signalled value "NS\_05") 96

6.6.3.3.2 Minimum requirement (network signalled value “NS\_07”) 96

6.6.3.3.3 Minimum requirement (network signalled value “NS\_08”) 96

6.6.3.3.4 Minimum requirement (network signalled value “NS\_09”) 97

6.6.3.3.5 Minimum requirement (network signalled value “NS\_12”) 97

6.6.3.3.6 Minimum requirement (network signalled value “NS\_13”) 97

6.6.3.3.7 Minimum requirement (network signalled value “NS\_14”) 98

6.6.3.3.8 Minimum requirement (network signalled value “NS\_15”) 98

6.6.3.3.9 Minimum requirement (network signalled value “NS\_16”) 98

6.6.3.3.10 Minimum requirement (network signalled value “NS\_17”) 99

6.6.3.3.11 Minimum requirement (network signalled value “NS\_18”) 99

6.6.3.3.12 Minimum requirement (network signalled value “NS\_19”) 99

6.6.3.3.13 Minimum requirement (network signalled value "NS\_11") 99

6.6.3.3.14 Minimum requirement (network signalled value " NS\_20") 100

6.6.3.3.15 Minimum requirement (network signalled value " NS\_22") 100

6.6.3.3.16 Minimum requirement (network signalled value “NS\_23”) 100

6.6.3.3.17 Void 101

6.6.3.3.18 Void 101

6.6.3.3.19 Void 101

6.6.3.3.20 Void 102

6.6.3.3.21 Void 102

6.6.3.3.22 Void 102

6.6.3.3.23 Void 102

6.6.3.3.24 Void 102

6.6.3.3.25 Void 102

6.6.3.3.26 Void 102

6.6.3.3.27 Void 102

6.6.3.3.28 Void 102

6.6.3.3.29 Void 102

6.6.3.3.30 Void 102

6.6.3.3.31 Void 102

6.6.3.3.32 Void 103

6.6.3.3.33 Void 103

6.6.3.3.34 Void 103

6.6.3.3.35 Minimum requirement (network signalled value “NS\_56”) 103

6.6.3.3A Additional spurious emissions for CA 103

6.6.3.3A.1 Minimum requirement for CA\_1C (network signalled value "CA\_NS\_01") 103

6.6.3.3A.2 Minimum requirement for CA\_1C (network signalled value "CA\_NS\_02") 104

6.6.3.3A.3 Minimum requirement for CA\_1C (network signalled value "CA\_NS\_03") 104

6.6.3.3A.4 Minimum requirement for CA\_38C (network signalled value "CA\_NS\_05") 104

6.6.3.3A.5 Minimum requirement for CA\_7C (network signalled value "CA\_NS\_06") 105

6.6.3.3A.6 Void 105

6.6.3.3A.7 Void 105

6.6.3.3A.8 Minimum requirement for CA\_41C (network signalled value "CA\_NS\_04") 105

6.6.3A Void 105

6.6.3B Spurious emission for UL-MIMO 105

6.6A Void 106

6.6B Void 106

6.7 Transmit intermodulation 106

6.7.1 Minimum requirement 106

6.7.1A Minimum requirement for CA 106

6.7.1B Minimum requirement for UL-MIMO 107

6.8 Void 107

6.8.1 Void 107

6.8A Void 107

6.8B Time alignment error for UL-MIMO 107

6.8B.1 Minimum Requirements 107

7 Receiver characteristics 107

7.1 General 107

7.2 Diversity characteristics 108

7.3 Reference sensitivity power level 108

7.3.1 Minimum requirements (QPSK) 108

7.3.1A Minimum requirements (QPSK) for CA 115

7.3.1B Minimum requirements (QPSK) for UL-MIMO 118

7.3.2 Void 118

7.4 Maximum input level 118

7.4.1 Minimum requirements 118

7.4.1A Minimum requirements for CA 119

7.4.1B Minimum requirements for UL-MIMO 120

7.4A Void 120

7.4A.1 Void 120

7.5 Adjacent Channel Selectivity (ACS) 120

7.5.1 Minimum requirements 120

7.5.1A Minimum requirements for CA 121

7.5.1B Minimum requirements for UL-MIMO 122

7.6 Blocking characteristics 122

7.6.1 In-band blocking 122

7.6.1.1 Minimum requirements 123

7.6.1.1A Minimum requirements for CA 123

7.6.2 Out-of-band blocking 125

7.6.2.1 Minimum requirements 125

7.6.2.1A Minimum requirements for CA 126

7.6.3 Narrow band blocking 127

7.6.3.1 Minimum requirements 127

7.6.3.1A Minimum requirements for CA 128

7.6A Void 129

7.6B Blocking characteristics for UL-MIMO 129

7.7 Spurious response 129

7.7.1 Minimum requirements 129

7.7.1A Minimum requirements for CA 130

7.7.1B Minimum requirements for UL-MIMO 131

7.8 Intermodulation characteristics 131

7.8.1 Wide band intermodulation 131

7.8.1.1 Minimum requirements 131

7.8.1A Minimum requirements for CA 131

7.8.1B Minimum requirements for UL-MIMO 132

7.8.2 Void 133

7.9 Spurious emissions 133

7.9.1 Minimum requirements 133

7.9.1A Minimum requirements 133

7.10 Receiver image 133

7.10.1 Void 133

7.10.1A Minimum requirements for CA 133

8 Performance requirement 135

8.1 General 135

8.1.1 Dual-antenna receiver capability 135

8.1.1.1 Simultaneous unicast and MBMS operations 135

8.1.1.2 Dual-antenna receiver capability in idle mode 135

8.1.2 Applicability of requirements 135

8.1.2.1 Applicability of requirements for different channel bandwidths 135

8.1.2.2 Definition of CA capability 135

8.1.2.3 Applicability and test rules for different CA configurations and bandwidth combination sets 136

8.1.2.4 Test coverage for different number of component carriers 137

8.2 Demodulation of PDSCH (Cell-Specific Reference Symbols) 138

8.2.1 FDD (Fixed Reference Channel) 138

8.2.1.1 Single-antenna port performance 138

8.2.1.1.1 Minimum Requirement 138

8.2.1.1.2 Void 141

8.2.1.1.3 Void 141

8.2.1.1.4 Minimum Requirement 1 PRB allocation in presence of MBSFN 141

8.2.1.2 Transmit diversity performance 141

8.2.1.2.1 Minimum Requirement 2 Tx Antenna Port 141

8.2.1.2.2 Minimum Requirement 4 Tx Antenna Port 142

8.2.1.2.3 Minimum Requirement 2 Tx Antenna Ports (demodulation subframe overlaps with aggressor cell ABS) 143

8.2.1.2.3A Minimum Requirement 2 Tx Antenna Ports (demodulation subframe overlaps with aggressor cell ABS and CRS assistance information are configured) 145

8.2.1.2.4 Enhanced Performance Requirement Type A - 2 Tx Antenna Ports with TM3 interference model 147

8.2.1.3 Open-loop spatial multiplexing performance 149

8.2.1.3.1 Minimum Requirement 2 Tx Antenna Port 149

8.2.1.3.1A Soft buffer management test 150

8.2.1.3.2 Minimum Requirement 4 Tx Antenna Port 151

8.2.1.3.3 Minimum Requirement 2 Tx Antenna Port (demodulation subframe overlaps with aggressor cell ABS) 152

8.2.1.3.4 Minimum Requirement 2 Tx Antenna Port (demodulation subframe overlaps with aggressor cell ABS and CRS assistance information are configured) 156

8.2.1.4 Closed-loop spatial multiplexing performance 158

8.2.1.4.1 Minimum Requirement Single-Layer Spatial Multiplexing 2 Tx Antenna Port 158

8.2.1.4.1A Minimum Requirement Single-Layer Spatial Multiplexing 4 Tx Antenna Port 159

8.2.1.4.1B Enhanced Performance Requirement Type A - Single-Layer Spatial Multiplexing 2 Tx Antenna Port with TM4 interference model 159

8.2.1.4.1C Minimum Requirement Single-Layer Spatial Multiplexing 2 Tx Antenna Ports (demodulation subframe overlaps with aggressor cell ABS and CRS assistance information are configured) 161

8.2.1.4.2 Minimum Requirement Multi-Layer Spatial Multiplexing 2 Tx Antenna Port 164

8.2.1.4.3 Minimum Requirement Multi-Layer Spatial Multiplexing 4 Tx Antenna Port 165

8.2.1.5 MU-MIMO 167

8.2.1.6 [Control channel performance: D-BCH and PCH] 167

8.2.1.7 Carrier aggregation with power imbalance 167

8.2.1.7.1 Minimum Requirement 167

8.2.1.8 Intra-band non-contiguous carrier aggregation with timing offset 168

8.2.1.8.1 Minimum Requirement 168

8.2.2 TDD (Fixed Reference Channel) 169

8.2.2.1 Single-antenna port performance 170

8.2.2.1.1 Minimum Requirement 170

8.2.2.1.2 Void 173

8.2.2.1.3 Void 173

8.2.2.1.4 Minimum Requirement 1 PRB allocation in presence of MBSFN 173

8.2.2.2 Transmit diversity performance 173

8.2.2.2.1 Minimum Requirement 2 Tx Antenna Port 173

8.2.2.2.2 Minimum Requirement 4 Tx Antenna Port 174

8.2.2.2.3 Minimum Requirement 2 Tx Antenna Port (demodulation subframe overlaps with aggressor cell ABS) 175

8.2.2.2.3A Minimum Requirement 2 Tx Antenna Ports (demodulation subframe overlaps with aggressor cell ABS and CRS assistance information are configured) 176

8.2.2.2.4 Enhanced Performance Requirement Type A – 2 Tx Antenna Ports with TM3 interference model 178

8.2.2.3 Open-loop spatial multiplexing performance 180

8.2.2.3.1 Minimum Requirement 2 Tx Antenna Port 180

8.2.2.3.1A Soft buffer management test 181

8.2.2.3.2 Minimum Requirement 4 Tx Antenna Port 181

8.2.2.3.3 Minimum Requirement 2Tx antenna port (demodulation subframe overlaps with aggressor cell ABS) 182

8.2.2.3.4 Minimum Requirement 2 Tx Antenna Port (demodulation subframe overlaps with aggressor cell ABS and CRS assistance information are configured) 186

8.2.2.4 Closed-loop spatial multiplexing performance 188

8.2.2.4.1 Minimum Requirement Single-Layer Spatial Multiplexing 2 Tx Antenna Port 188

8.2.2.4.1A Minimum Requirement Single-Layer Spatial Multiplexing 4 Tx Antenna Port 189

8.2.2.4.1B Enhanced Performance Requirement Type A – Single-Layer Spatial Multiplexing 2 Tx Antenna Port with TM4 interference model 189

8.2.2.4.1C Minimum Requirement Single-Layer Spatial Multiplexing 2 Tx Antenna Ports (demodulation subframe overlaps with aggressor cell ABS and CRS assistance information are configured) 191

8.2.2.4.2 Minimum Requirement Multi-Layer Spatial Multiplexing 2 Tx Antenna Port 193

8.2.2.4.3 Minimum Requirement Multi-Layer Spatial Multiplexing 4 Tx Antenna Port 194

8.2.2.5 MU-MIMO 195

8.2.2.6 [Control channel performance: D-BCH and PCH] 195

8.2.2.7 Carrier aggregation with power imbalance 195

8.2.2.7.1 Minimum Requirement 195

8.3 Demodulation of PDSCH (User-Specific Reference Symbols) 196

8.3.1 FDD 196

8.3.1.1 Single-layer Spatial Multiplexing 197

8.3.1.1A Enhanced Performance Requirement Type A – Single-layer Spatial Multiplexing with TM9 interference model 199

8.3.1.1B Single-layer Spatial Multiplexing (demodulation subframe overlaps with aggressor cell ABS and CRS assistance information are configured) 202

8.3.1.2 Dual-Layer Spatial Multiplexing 205

8.3.1.3 Performance requirements for DCI format 2D and non Quasi Co-located Antenna Ports 206

8.3.1.3.1 Minimum requirement with Same Cell ID (with single NZP CSI-RS resource) 206

8.3.1.3.2 Minimum requirements with Same Cell ID (with multiple NZP CSI-RS resources) 208

8.3.1.3.3 Minimum requirement with Different Cell ID and Colliding CRS (with single NZP CSI-RS resource) 210

8.3.2 TDD 212

8.3.2.1 Single-layer Spatial Multiplexing 212

8.3.2.1A Single-layer Spatial Multiplexing (with multiple CSI-RS configurations) 214

8.3.2.1B Enhanced Performance Requirement Type A – Single-layer Spatial Multiplexing with TM9 interference model 216

8.3.2.1C Single-layer Spatial Multiplexing (demodulation subframe overlaps with aggressor cell ABS and CRS assistance information are configured) 219

8.3.2.2 Dual-Layer Spatial Multiplexing 222

8.3.2.3 Dual-Layer Spatial Multiplexing (with multiple CSI-RS configurations) 223

8.3.2.4 Performance requirements for DCI format 2D and non Quasi Co-located Antenna Ports 224

8.3.2.4.1 Minimum requirement with Same Cell ID (with single NZP CSI-RS resource) 224

8.3.2.4.2 Minimum requirements with Same Cell ID (with multiple NZP CSI-RS resources) 226

8.3.2.4.3 Minimum requirement with Different Cell ID and Colliding CRS (with single NZP CSI-RS resource) 228

8.4 Demodulation of PDCCH/PCFICH 230

8.4.1 FDD 230

8.4.1.1 Single-antenna port performance 230

8.4.1.2 Transmit diversity performance 230

8.4.1.2.1 Minimum Requirement 2 Tx Antenna Port 230

8.4.1.2.2 Minimum Requirement 4 Tx Antenna Port 231

8.4.1.2.3 Minimum Requirement 2 Tx Antenna Port (demodulation subframe overlaps with aggressor cell ABS) 231

8.4.1.2.4 Minimum Requirement 2 Tx Antenna Port (demodulation subframe overlaps with aggressor cell ABS and CRS assistance information are configured) 236

8.4.2 TDD 241

8.4.2.1 Single-antenna port performance 242

8.4.2.2 Transmit diversity performance 242

8.4.2.2.1 Minimum Requirement 2 Tx Antenna Port 242

8.4.2.2.2 Minimum Requirement 4 Tx Antenna Port 243

8.4.2.2.3 Minimum Requirement 2 Tx Antenna Port (demodulation subframe overlaps with aggressor cell ABS) 243

8.4.2.2.4 Minimum Requirement 2 Tx Antenna Port (demodulation subframe overlaps with aggressor cell ABS and CRS assistance information are configured) 247

8.5 Demodulation of PHICH 251

8.5.1 FDD 251

8.5.1.1 Single-antenna port performance 251

8.5.1.2 Transmit diversity performance 252

8.5.1.2.1 Minimum Requirement 2 Tx Antenna Port 252

8.5.1.2.2 Minimum Requirement 4 Tx Antenna Port 252

8.5.1.2.3 Minimum Requirement 2 Tx Antenna Port (demodulation subframe overlaps with aggressor cell ABS) 252

8.5.1.2.4 Minimum Requirement 2 Tx Antenna Port (demodulation subframe overlaps with aggressor cell ABS and CRS assistance information are configured) 254

8.5.2 TDD 257

8.5.2.1 Single-antenna port performance 258

8.5.2.2 Transmit diversity performance 258

8.5.2.2.1 Minimum Requirement 2 Tx Antenna Port 258

8.5.2.2.2 Minimum Requirement 4 Tx Antenna Port 259

8.5.2.2.3 Minimum Requirement 2 Tx Antenna Port (demodulation subframe overlaps with aggressor cell ABS) 259

8.5.2.2.4 Minimum Requirement 2 Tx Antenna Port (demodulation subframe overlaps with aggressor cell ABS and CRS assistance information are configured) 261

8.6 Demodulation of PBCH 263

8.6.1 FDD 263

8.6.1.1 Single-antenna port performance 263

8.6.1.2 Transmit diversity performance 264

8.6.1.2.1 Minimum Requirement 2 Tx Antenna Port 264

8.6.1.2.2 Minimum Requirement 4 Tx Antenna Port 264

8.6.1.2.3 Minimum Requirement 2 Tx Antenna Port under Time Domain Measurement Resource Restriction with CRS Assistance Information 264

8.6.2 TDD 266

8.6.2.1 Single-antenna port performance 266

8.6.2.2 Transmit diversity performance 266

8.6.2.2.1 Minimum Requirement 2 Tx Antenna Port 266

8.6.2.2.2 Minimum Requirement 4 Tx Antenna Port 266

8.6.2.2.3 Minimum Requirement 2 Tx Antenna Port under Time Domain Measurement Resource Restriction with CRS Assistance Information 267

8.7 Sustained downlink data rate provided by lower layers 268

8.7.1 FDD 268

8.7.2 TDD 270

8.7.3 FDD (EPDCCH scheduling) 271

8.7.4 TDD (EPDCCH scheduling) 273

8.8 Demodulation of EPDCCH 275

8.8.1 Distributed Transmission 275

8.8.1.1 FDD 275

8.8.1.1.1 Void 276

8.8.1.2 TDD 276

8.8.1.2.1 Void 277

8.8.2 Localized Transmission with TM9 277

8.8.2.1 FDD 277

8.8.2.1.1 Void 278

8.8.2.1.2 Void 279

8.8.2.2 TDD 279

8.8.2.2.1 Void 280

8.8.2.2.2 Void 280

8.8.3 Localized transmission with TM10 Type B quasi co-location type 280

8.8.3.1 FDD 280

8.8.3.2 TDD 283

9 Reporting of Channel State Information 286

9.1 General 286

9.1.1 Applicability of requirements 286

9.1.1.1 Applicability of requirements for different channel bandwidths 286

9.1.1.2 Applicability and test rules for different CA configurations and bandwidth combination sets 286

9.2 CQI reporting definition under AWGN conditions 287

9.2.1 Minimum requirement PUCCH 1-0 (Cell-Specific Reference Symbols) 287

9.2.1.1 FDD 287

9.2.1.2 TDD 288

9.2.1.3 FDD (CSI measurements in case two CSI subframe sets are configured) 289

9.2.1.4 TDD (CSI measurements in case two CSI subframe sets are configured) 292

9.2.1.5 FDD (CSI measurements in case two CSI subframe sets are configured and with CRS assistance information) 295

9.2.1.6 TDD (CSI measurements in case two CSI subframe sets are configured and with CRS assistance information) 298

9.2.2 Minimum requirement PUCCH 1-1 (Cell-Specific Reference Symbols) 301

9.2.2.1 FDD 301

9.2.2.2 TDD 302

9.2.3 Minimum requirement PUCCH 1-1 (CSI Reference Symbols) 303

9.2.3.1 FDD 303

9.2.3.2 TDD 304

9.2.4 Minimum requirement PUCCH 1-1 (With Single CSI Process) 305

9.2.4.1 FDD 305

9.2.4.2 TDD 308

9.3 CQI reporting under fading conditions 311

9.3.1 Frequency-selective scheduling mode 311

9.3.1.1 Minimum requirement PUSCH 3-0 (Cell-Specific Reference Symbols) 311

9.3.1.1.1 FDD 311

9.3.1.1.2 TDD 312

9.3.1.1.3 FDD (CSI measurements in case two CSI subframe sets are configured and with CRS assistance information) 313

9.3.1.1.4 TDD (CSI measurements in case two CSI subframe sets are configured and with CRS assistance information) 317

9.3.1.2 Minimum requirement PUSCH 3-1 (CSI Reference Symbol) 320

9.3.1.2.1 FDD 320

9.3.1.2.2 TDD 321

9.3.2 Frequency non-selective scheduling mode 323

9.3.2.1 Minimum requirement PUCCH 1-0 (Cell-Specific Reference Symbol) 323

9.3.2.1.1 FDD 323

9.3.2.1.2 TDD 324

9.3.2.2 Minimum requirement PUCCH 1-1 (CSI Reference Symbol) 326

9.3.2.2.1 FDD 326

9.3.2.2.2 TDD 327

9.3.3 Frequency-selective interference 329

9.3.3.1 Minimum requirement PUSCH 3-0 (Cell-Specific Reference Symbol) 329

9.3.3.1.1 FDD 329

9.3.3.1.2 TDD 330

9.3.3.2 Void 331

9.3.3.2.1 Void 331

9.3.3.2.2 Void 331

9.3.4 UE-selected subband CQI 331

9.3.4.1 Minimum requirement PUSCH 2-0 (Cell-Specific Reference Symbols) 331

9.3.4.1.1 FDD 331

9.3.4.1.2 TDD 332

9.3.4.2 Minimum requirement PUCCH 2-0 (Cell-Specific Reference Symbols) 333

9.3.4.2.1 FDD 333

9.3.4.2.2 TDD 335

9.3.5 Additional requirements for enhanced receiver Type A 337

9.3.5.1 Minimum requirement PUCCH 1-0 (Cell-Specific Reference Symbol) 337

9.3.5.1.1 FDD 337

9.3.5.1.2 TDD 338

9.3.5.2 Minimum requirement PUCCH 1-1 (CSI Reference Symbol) 341

9.3.5.2.1 FDD 341

9.3.5.2.2 TDD 344

9.3.6 Minimum requirement (With multiple CSI processes) 347

9.3.6.1 FDD 348

9.3.6.2 TDD 352

9.4 Reporting of Precoding Matrix Indicator (PMI) 356

9.4.1 Single PMI 357

9.4.1.1 Minimum requirement PUSCH 3-1 (Cell-Specific Reference Symbols) 357

9.4.1.1.1 FDD 357

9.4.1.1.2 TDD 357

9.4.1.2 Minimum requirement PUCCH 2-1 (Cell-Specific Reference Symbols) 358

9.4.1.2.1 FDD 358

9.4.1.2.2 TDD 360

9.4.1.3 Minimum requirement PUSCH 3-1 (CSI Reference Symbol) 361

9.4.1.3.1 FDD 361

9.4.1.3.2 TDD 362

9.4.1a Void 365

9.4.1a.1 Void 365

9.4.1a.1.1 Void 365

9.4.1a.1.2 Void 365

9.4.2 Multiple PMI 365

9.4.2.1 Minimum requirement PUSCH 1-2 (Cell-Specific Reference Symbols) 365

9.4.2.1.1 FDD 365

9.4.2.1.2 TDD 366

9.4.2.2 Minimum requirement PUSCH 2-2 (Cell-Specific Reference Symbols) 367

9.4.2.2.1 FDD 367

9.4.2.2.2 TDD 368

9.4.2.3 Minimum requirement PUSCH 1-2 (CSI Reference Symbol) 369

9.4.2.3.1 FDD 369

9.4.2.3.2 TDD 371

9.4.3 Void 374

9.4.3.1 Void 374

9.4.3.1.1 Void 374

9.4.3.1.2 Void 374

9.5 Reporting of Rank Indicator (RI) 374

9.5.1 Minimum requirement (Cell-Specific Reference Symbols) 374

9.5.1.1 FDD 374

9.5.1.2 TDD 376

9.5.2 Minimum requirement (CSI Reference Symbols) 377

9.5.2.1 FDD 377

9.5.2.2 TDD 379

9.5.3 Minimum requirement (CSI measurements in case two CSI subframe sets are configured) 381

9.5.3.1 FDD 381

9.5.3.2 TDD 384

9.5.4 Minimum requirement (CSI measurements in case two CSI subframe sets are configured and CRS assistance information are configured) 387

9.5.4.1 FDD 387

9.5.4.2 TDD 390

9.5.5 Minimum requirement (with CSI process) 393

9.5.5.1 FDD 394

9.5.5.2 TDD 397

9.6 Additional requirements for carrier aggregation 400

9.6.1 Periodic reporting on multiple cells (Cell-Specific Reference Symbols) 400

9.6.1.1 FDD 400

9.6.1.2 TDD 401

10 Performance requirement (MBMS) 402

10.1 FDD (Fixed Reference Channel) 402

10.1.1 Minimum requirement 403

10.2 TDD (Fixed Reference Channel) 403

10.2.1 Minimum requirement 404

Annex A (normative): Measurement channels 405

A.1 General 405

A.2 UL reference measurement channels 405

A.2.1 General 405

A.2.1.1 Applicability and common parameters 405

A.2.1.2 Determination of payload size 405

A.2.1.3 Overview of UL reference measurement channels 406

A.2.2 Reference measurement channels for FDD 411

A.2.2.1 Full RB allocation 411

A.2.2.1.1 QPSK 411

A.2.2.1.2 16-QAM 412

A.2.2.1.3 64-QAM 412

A.2.2.2 Partial RB allocation 412

A.2.2.2.1 QPSK 413

A.2.2.2.2 16-QAM 414

A.2.2.2.3 64-QAM 414

A.2.2.3 Void 414

A.2.3 Reference measurement channels for TDD 414

A.2.3.1 Full RB allocation 415

A.2.3.1.1 QPSK 415

A.2.3.1.2 16-QAM 415

A.2.3.1.3 64-QAM 415

A.2.3.2 Partial RB allocation 416

A.2.3.2.1 QPSK 416

A.2.3.2.2 16-QAM 417

A.2.3.2.3 64-QAM 417

A.2.3.3 Void 417

A.3 DL reference measurement channels 417

A.3.1 General 417

A.3.1.1 Overview of DL reference measurement channels 418

A.3.2 Reference measurement channel for receiver characteristics 426

A.3.3 Reference measurement channels for PDSCH performance requirements (FDD) 433

A.3.3.1 Single-antenna transmission (Common Reference Symbols) 433

A.3.3.2 Multi-antenna transmission (Common Reference Symbols) 438

A.3.3.2.1 Two antenna ports 438

A.3.3.2.2 Four antenna ports 441

A.3.3.3 Reference Measurement Channel for UE-Specific Reference Symbols 441

A.3.3.3.1 Two antenna port (CSI-RS) 441

A.3.3.3.2 Four antenna ports (CSI-RS) 443

A.3.4 Reference measurement channels for PDSCH performance requirements (TDD) 446

A.3.4.1 Single-antenna transmission (Common Reference Symbols) 446

A.3.4.2 Multi-antenna transmission (Common Reference Signals) 454

A.3.4.2.1 Two antenna ports 454

A.3.4.2.2 Four antenna ports 456

A.3.4.3 Reference Measurement Channels for UE-Specific Reference Symbols 456

A.3.4.3.1 Single antenna port (Cell Specific) 456

A.3.4.3.2 Two antenna ports (Cell Specific) 457

A.3.4.3.3 Two antenna ports (CSI-RS) 458

A.3.4.3.4 Four antenna ports (CSI-RS) 460

A.3.4.3.5 Eight antenna ports (CSI-RS) 461

A.3.5 Reference measurement channels for PDCCH/PCFICH performance requirements 464

A.3.5.1 FDD 464

A.3.5.2 TDD 464

A.3.6 Reference measurement channels for PHICH performance requirements 464

A.3.7 Reference measurement channels for PBCH performance requirements 465

A.3.8 Reference measurement channels for MBMS performance requirements 465

A.3.8.1 FDD 465

A.3.8.2 TDD 467

A.3.9 Reference measurement channels for sustained downlink data rate provided by lower layers 469

A.3.9.1 FDD 469

A.3.9.2 TDD 470

A.3.9.3 FDD (EPDCCH scheduling) 471

A.3.9.4 TDD (EPDCCH scheduling) 472

A.3.10 Reference Measurement Channels for EPDCCH performance requirements 473

A.3.10.1 FDD 473

A.3.10.2 TDD 473

A.4 CSI reference measurement channels 473

A.5 OFDMA Channel Noise Generator (OCNG) 480

A.5.1 OCNG Patterns for FDD 480

A.5.1.1 OCNG FDD pattern 1: One sided dynamic OCNG FDD pattern 481

A.5.1.2 OCNG FDD pattern 2: Two sided dynamic OCNG FDD pattern 481

A.5.1.3 OCNG FDD pattern 3: 49 RB OCNG allocation with MBSFN in 10 MHz 482

A.5.1.4 OCNG FDD pattern 4: One sided dynamic OCNG FDD pattern for MBMS transmission 482

A.5.1.5 OCNG FDD pattern 5: One sided dynamic 16QAM modulated OCNG FDD pattern 483

A.5.1.6 OCNG FDD pattern 6: dynamic OCNG FDD pattern when user data is in 2 non-contiguous blocks 484

A.5.1.7 OCNG FDD pattern 7: dynamic OCNG FDD pattern when user data is in multiple non-contiguous blocks 484

A.5.1.8 OCNG FDD pattern 8: Dynamic OCNG FDD pattern for TM10 transmission 485

A.5.2 OCNG Patterns for TDD 486

A.5.2.1 OCNG TDD pattern 1: One sided dynamic OCNG TDD pattern 486

A.5.2.2 OCNG TDD pattern 2: Two sided dynamic OCNG TDD pattern 487

A.5.2.3 OCNG TDD pattern 3: 49 RB OCNG allocation with MBSFN in 10 MHz 488

A.5.2.4 OCNG TDD pattern 4: One sided dynamic OCNG TDD pattern for MBMS transmission 488

A.5.2.5 OCNG TDD pattern 5: One sided dynamic 16QAM modulated OCNG TDD pattern 489

A.5.2.6 OCNG TDD pattern 6: dynamic OCNG TDD pattern when user data is in 2 non-contiguous blocks 490

A.5.2.7 OCNG TDD pattern 7: dynamic OCNG TDD pattern when user data is in multiple non-contiguous blocks 490

A.5.2.8 OCNG TDD pattern 8: Dynamic OCNG TDD pattern for TM10 transmission 491

Annex B (normative): Propagation conditions 493

B.1 Static propagation condition 493

B.2 Multi-path fading propagation conditions 493

B.2.1 Delay profiles 493

B.2.2 Combinations of channel model parameters 494

B.2.3 MIMO Channel Correlation Matrices 495

B.2.3.1 Definition of MIMO Correlation Matrices 495

B.2.3.2 MIMO Correlation Matrices at High, Medium and Low Level 496

B.2.3A MIMO Channel Correlation Matrices using cross polarized antennas 498

B.2.3A.1 Definition of MIMO Correlation Matrices using cross polarized antennas 499

B.2.3A.2 Spatial Correlation Matrices using cross polarized antennas at eNB and UE sides 499

B.2.3A.2.1 Spatial Correlation Matrices at eNB side 499

B.2.3A.2.2 Spatial Correlation Matrices at UE side 500

B.2.3A.4 Beam steering approach 500

B.2.4 Propagation conditions for CQI tests 501

B.2.4.1 Propagation conditions for CQI tests with multiple CSI processes 501

B.2.5 Void 501

B.2.6 MBSFN Propagation Channel Profile 501

B.3 High speed train scenario 502

B.4 Beamforming Model 503

B.4.1 Single-layer random beamforming (Antenna port 5, 7, or 8) 503

B.4.2 Dual-layer random beamforming (antenna ports 7 and 8) 504

B.4.3 Generic beamforming model (antenna ports 7-14) 504

B.4.4 Random beamforming for EPDCCH distributed transmission (Antenna port 107 and 109) 505

B.4.5 Random beamforming for EPDCCH localized transmission (Antenna port 107, 108, 109 or 110) 505

B.5 Interference models for enhanced performance requirements Type-A 506

B.5.1 Dominant interferer proportion 506

B.5.2 Transmission mode 3 interference model 506

B.5.3 Transmission mode 4 interference model 507

B.5.4 Transmission mode 9 interference model 507

Annex C (normative): Downlink Physical Channels 508

C.1 General 508

C.2 Set-up 508

C.3 Connection 508

C.3.1 Measurement of Receiver Characteristics 508

C.3.2 Measurement of Performance requirements 509

C.3.3 Aggressor cell power allocation for Measurement of Performance Requirements when ABS is Configured 510

C.3.4 Power Allocation for Measurement of Performance Requirements when Quasi Co-location Type B: same Cell ID 511

Annex D (normative): Characteristics of the interfering signal 512

D.1 General 512

D.2 Interference signals 512

Annex E (normative): Environmental conditions 513

E.1 General 513

E.2 Environmental 513

E.2.1 Temperature 513

E.2.2 Voltage 513

E.2.3 Vibration 514

Annex F (normative): Transmit modulation 515

F.1 Measurement Point 515

F.2 Basic Error Vector Magnitude measurement 515

F.3 Basic in-band emissions measurement 516

F.4 Modified signal under test 516

F.5 Window length 518

F.5.1 Timing offset 518

F.5.2 Window length 518

F.5.3 Window length for normal CP 518

F.5.4 Window length for Extended CP 519

F.5.5 Window length for PRACH 519

F.6 Averaged EVM 520

F.7 Spectrum Flatness 521

Annex G (informative): Reference sensitivity level in lower SNR 522

G.1 General 522

G.2 Typical receiver sensitivity performance (QPSK) 522

G.3 Reference measurement channel for REFSENSE in lower SNR 525

Annex H (normative): Modified MPR behavior 526

H.1 Indication of modified MPR behavior 526

Annex I (informative): Change history 528