3GPP TS 36.101 V12.31.0 (2023-03)

Technical Specification

3rd Generation Partnership Project;

Technical Specification Group Radio Access Network;

Evolved Universal Terrestrial Radio Access (E-UTRA);

User Equipment (UE) radio transmission and reception

(Release 12)

 

The present document has been developed within the 3rd Generation Partnership Project (3GPP TM) and may be further elaborated for the purposes of 3GPP.  
The present document has not been subject to any approval process by the 3GPPOrganizational Partners and shall not be implemented.   
This Specification is provided for future development work within 3GPPonly. The Organizational Partners accept no liability for any use of this Specification.  
Specifications and reports for implementation of the 3GPP TM system should be obtained via the 3GPP Organizational Partners' Publications Offices.

***3GPP***

Postal address

3GPP support office address

650 Route des Lucioles - Sophia Antipolis

Valbonne - FRANCE

Tel.: +33 4 92 94 42 00 Fax: +33 4 93 65 47 16

Internet

http://www.3gpp.org

***Copyright Notification***

No part may be reproduced except as authorized by written permission.  
The copyright and the foregoing restriction extend to reproduction in all media.

© 2023, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

All rights reserved.

UMTS™ is a Trade Mark of ETSI registered for the benefit of its members

3GPP™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners  
LTE™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners

GSM® and the GSM logo are registered and owned by the GSM Association

Contents

Foreword 19

1 Scope 20

2 References 20

3 Definitions, symbols and abbreviations 20

3.1 Definitions 20

3.2 Symbols 22

3.3 Abbreviations 24

4 General 25

4.1 Relationship between minimum requirements and test requirements 25

4.2 Applicability of minimum requirements 26

4.3 Void 26

4.3A Applicability of minimum requirements (CA, UL-MIMO, ProSe, Dual Connectivity, UE category 0) 26

4.4 RF requirements in later releases 27

5 Operating bands and channel arrangement 27

5.1 General 27

5.2 Void 27

5.3 Void 27

5.4 Void 27

5.5 Operating bands 27

5.5A Operating bands for CA 30

5.5B Operating bands for UL-MIMO 37

5.5C Operating bands for Dual Connectivity 37

5.5D Operating bands for ProSe 39

5.5E Operating bands for UE category 0 39

5.6 Channel bandwidth 39

5.6.1 Channel bandwidths per operating band 40

5.6A Channel bandwidth for CA 41

5.6A.1 Channel bandwidths per operating band for CA 44

5.6B Channel bandwidth for UL-MIMO 57

5.6B.1 Void 57

5.6C Channel bandwidth for Dual Connectivity 57

NOTE 2: For TDD inter-band dual connectivity configurations, requirements are applicable only for synchronous operation.5.6C.1 Void 58

5.6D Channel bandwidth for ProSe 58

5.6D.1 Channel bandwidths per operating band for ProSe 58

5.7 Channel arrangement 58

5.7.1 Channel spacing 58

5.7.1A Channel spacing for CA 59

5.7.2 Channel raster 59

5.7.2A Channel raster for CA 59

5.7.3 Carrier frequency and EARFCN 59

5.7.4 TX–RX frequency separation 60

5.7.4A TX–RX frequency separation for CA 61

6 Transmitter characteristics 61

6.1 General 61

6.2 Transmit power 62

6.2.1 Void 62

6.2.2 UE maximum output power 62

6.2.2A UE maximum output power for CA 63

6.2.2B UE maximum output power for UL-MIMO 65

6.2.3 UE maximum output power for modulation / channel bandwidth 67

6.2.3A UE Maximum Output power for modulation / channel bandwidth for CA 67

6.2.3B UE maximum output power for modulation / channel bandwidth for UL-MIMO 69

6.2.3D UE maximum output power for modulation / channel bandwidth for ProSe 69

6.2.4 UE maximum output power with additional requirements 69

6.2.4A UE maximum output power with additional requirements for CA 78

6.2.4A.1 A-MPR for CA\_NS\_01 for CA\_1C 80

6.2.4A.2 A-MPR for CA\_NS\_02 for CA\_1C 80

6.2.4A.3 A-MPR for CA\_NS\_03 for CA\_1C 81

6.2.4A.4 A-MPR for CA\_NS\_04 82

6.2.4A.5 A-MPR for CA\_NS\_05 for CA\_38C 82

6.2.4A.6 A-MPR for CA\_NS\_06 83

6.2.4A.7 A-MPR for CA\_NS\_07 84

6.2.4A.8 A-MPR for CA\_NS\_08 85

6.2.4B UE maximum output power with additional requirements for UL-MIMO 86

6.2.4D UE maximum output power with additional requirements for ProSe 87

6.2.5 Configured transmitted power 87

6.2.5A Configured transmitted power for CA 96

6.2.5B Configured transmitted power for UL-MIMO 98

6.2.5C Configured transmitted power for Dual Connectivity 99

6.2.5D Configured transmitted power for ProSe 100

6.3 Output power dynamics 101

6.3.1 (Void) 101

6.3.2 Minimum output power 101

6.3.2.1 Minimum requirement 101

6.3.2A UE Minimum output power for CA 101

6.3.2A.1 Minimum requirement for CA 101

6.3.2B UE Minimum output power for UL-MIMO 101

6.3.2B.1 Minimum requirement 102

6.3.3 Transmit OFF power 102

6.3.3.1. Minimum requirement 102

6.3.3A UE Transmit OFF power for CA 102

6.3.3A.1 Minimum requirement for CA 102

6.3.3B UE Transmit OFF power for UL-MIMO 103

6.3.3B.1 Minimum requirement 103

6.3.3D Transmit OFF power for ProSe 103

6.3.4 ON/OFF time mask 103

6.3.4.1 General ON/OFF time mask 103

6.3.4.2 PRACH and SRS time mask 104

6.3.4.2.1 PRACH time mask 104

6.3.4.2.2 SRS time mask 104

6.3.4.3 Slot / Sub frame boundary time mask 105

6.3.4.4 PUCCH / PUSCH / SRS time mask 106

6.3.4A ON/OFF time mask for CA 107

6.3.4B ON/OFF time mask for UL-MIMO 107

6.3.4D ON/OFF time mask for ProSe 107

6.3.4D.1 General time mask for ProSe 107

6.3.4D.2 PSSS/SSSS time mask 108

6.3.4D.3 PSSS / SSSS / PSBCH time mask 109

6.3.4D.4 PSSCH / SRS time mask 110

6.3.5 Power Control 110

6.3.5.1 Absolute power tolerance 110

6.3.5.1.1 Minimum requirements 110

6.3.5.2 Relative Power tolerance 110

6.3.5.2.1 Minimum requirements 110

6.3.5.3 Aggregate power control tolerance 111

6.3.5.3.1 Minimum requirement 111

6.3.5A Power control for CA 112

6.3.5A.1 Absolute power tolerance 112

6.3.5A.1.1 Minimum requirements 112

6.3.5A.2 Relative power tolerance 112

6.3.5A.2.1 Minimum requirements 112

6.3.5A.3 Aggregate power control tolerance 113

6.3.5A.3.1 Minimum requirements 113

6.3.5B Power control for UL-MIMO 113

6.3.5D Power Control for ProSe 113

6.3.5D.1 Absolute power tolerance 113

6.4 Void 114

6.5 Transmit signal quality 114

6.5.1 Frequency error 114

6.5.1A Frequency error for CA 114

6.5.1B Frequency error for UL-MIMO 114

6.5.1D Frequency error for ProSe 114

6.5.2 Transmit modulation quality 114

6.5.2.1 Error Vector Magnitude 114

6.5.2.1.1 Minimum requirement 115

6.5.2.2 Carrier leakage 115

6.5.2.2.1 Minimum requirements 115

6.5.2.3 In-band emissions 115

6.5.2.3.1 Minimum requirements 116

6.5.2.4 EVM equalizer spectrum flatness 116

6.5.2.4.1 Minimum requirements 116

6.5.2A Transmit modulation quality for CA 117

6.5.2A.1 Error Vector Magnitude 118

6.5.2A.2 Carrier leakage for CA 118

6.5.2A.2.1 Minimum requirements 118

6.5.2A.3 In-band emissions 118

6.5.2A.3.1 Minimum requirement for CA 118

6.5.2B Transmit modulation quality for UL-MIMO 120

6.5.2B.1 Error Vector Magnitude 121

6.5.2B.2 Carrier leakage 121

6.5.2B.3 In-band emissions 121

6.5.2B.4 EVM equalizer spectrum flatness for UL-MIMO 121

6.5.2D Transmit modulation quality for ProSe 121

6.5.2D.1 Error Vector Magnitude 121

6.5.2D.2 Carrier leakage 121

6.5.2D.3 In-band emissions 121

6.5.2D.4 EVM equalizer spectrum flatness for ProSe 122

6.6 Output RF spectrum emissions 122

6.6.1 Occupied bandwidth 122

6.6.1A Occupied bandwidth for CA 122

6.6.1B Occupied bandwidth for UL-MIMO 123

6.6.2 Out of band emission 123

6.6.2.1 Spectrum emission mask 123

6.6.2.1.1 Minimum requirement 123

6.6.2.1A Spectrum emission mask for CA 124

6.6.2.2 Additional spectrum emission mask 124

6.6.2.2.1 Minimum requirement (network signalled value "NS\_03", “NS\_11”, "NS\_20", and “NS\_21”) 124

6.6.2.2.2 Minimum requirement (network signalled value "NS\_04") 125

6.6.2.2.3 Minimum requirement (network signalled value "NS\_06" or “NS\_07”) 125

6.6.2.2A Additional Spectrum Emission Mask for CA 126

6.6.2.2A.1 Minimum requirement (network signalled value "CA\_NS\_04") 126

6.6.2.3 Adjacent Channel Leakage Ratio 127

6.6.2.3.1 Minimum requirement E-UTRA 127

6.6.2.3.1A Void 128

6.6.2.3.1Aa Void 128

6.6.2.3.2 Minimum requirements UTRA 128

6.6.2.3.2A Minimum requirement UTRA for CA 128

6.6.2.3.3A Minimum requirements for CA E-UTRA 130

6.6.2.4 Void 130

6.6.2.4.1 Void 130

6.6.2A Void 130

6.6.2B Out of band emission for UL-MIMO 131

6.6.3 Spurious emissions 131

6.6.3.1 Minimum requirements 131

6.6.3.1A Minimum requirements for CA 131

6.6.3.2 Spurious emission band UE co-existence 132

6.6.3.2A Spurious emission band UE co-existence for CA 138

6.6.3.3 Additional spurious emissions 145

6.6.3.3.1 Minimum requirement (network signalled value "NS\_05") 145

6.6.3.3.2 Minimum requirement (network signalled value “NS\_07”) 145

6.6.3.3.3 Minimum requirement (network signalled value “NS\_08”) 146

6.6.3.3.4 Minimum requirement (network signalled value “NS\_09”) 146

6.6.3.3.5 Minimum requirement (network signalled value "NS\_12") 146

6.6.3.3.6 Minimum requirement (network signalled value “NS\_13”) 146

6.6.3.3.7 Minimum requirement (network signalled value “NS\_14”) 147

6.6.3.3.8 Minimum requirement (network signalled value “NS\_15”) 147

6.6.3.3.9 Minimum requirement (network signalled value “NS\_16”) 147

6.6.3.3.10 Minimum requirement (network signalled value “NS\_17”) 148

6.6.3.3.11 Minimum requirement (network signalled value “NS\_18”) 148

6.6.3.3.12 Minimum requirement (network signalled value “NS\_19”) 148

6.6.3.3.13 Minimum requirement (network signalled value “NS\_11”) 148

6.6.3.3.14 Minimum requirement (network signalled value “NS\_20”) 149

6.6.3.3.15 Minimum requirement (network signalled value “NS\_21”) 149

6.6.3.3.16 Minimum requirement (network signalled value "NS\_22") 149

6.6.3.3.17 Minimum requirement (network signalled value “NS\_23”) 150

6.6.3.3.18 Void 150

6.6.3.3.19 Minimum requirement (network signalled value "NS\_04") 150

6.6.3.3.20 Void 152

6.6.3.3.21 Void 152

6.6.3.3.22 Void 152

6.6.3.3.23 Void 152

6.6.3.3.24 Void 152

6.6.3.3.25 Void 152

6.6.3.3.26 Void 152

6.6.3.3.27 Void 152

6.6.3.3.28 Void 152

6.6.3.3.29 Void 152

6.6.3.3.30 Void 152

6.6.3.3.31 Void 152

6.6.3.3.32 Void 153

6.6.3.3.33 Void 153

6.6.3.3.34 Void 153

6.6.3.3.35 Minimum requirement (network signalled value “NS\_56”) 153

6.6.3.3A Additional spurious emissions for CA 153

6.6.3.3A.1 Minimum requirement for CA\_1C (network signalled value "CA\_NS\_01") 153

6.6.3.3A.2 Minimum requirement for CA\_1C (network signalled value "CA\_NS\_02") 154

6.6.3.3A.3 Minimum requirement for CA\_1C (network signalled value "CA\_NS\_03") 154

6.6.3.3A.4 Minimum requirement for CA\_38C (network signalled value "CA\_NS\_05") 154

6.6.3.3A.5 Minimum requirement for CA\_7C (network signalled value "CA\_NS\_06") 155

6.6.3.3A.6 Minimum requirement for CA\_39C (network signalled value "CA\_NS\_07") 155

6.6.3.3A.7 Minimum requirement for CA\_42C (network signalled value "CA\_NS\_08") 155

6.6.3.3A.8 Minimum requirement for CA\_41C (network signalled value "CA\_NS\_04") 156

6.6.3A Void 156

6.6.3B Spurious emission for UL-MIMO 156

6.6A Void 157

6.6B Void 157

6.7 Transmit intermodulation 157

6.7.1 Minimum requirement 157

6.7.1A Minimum requirement for CA 157

6.7.1B Minimum requirement for UL-MIMO 158

6.8 Void 158

6.8.1 Void 158

6.8A Void 158

6.8B Time alignment error for UL-MIMO 158

6.8B.1 Minimum Requirements 158

7 Receiver characteristics 158

7.1 General 158

7.2 Diversity characteristics 159

7.3 Reference sensitivity power level 159

7.3.1 Minimum requirements (QPSK) 159

7.3.1A Minimum requirements (QPSK) for CA 173

7.3.1B Minimum requirements (QPSK) for UL-MIMO 189

7.3.1D Minimum requirements (QPSK) for ProSe 189

7.3.1E Minimum requirements (QPSK) for UE category 0 190

7.3.2 Void 191

7.4 Maximum input level 191

7.4.1 Minimum requirements 191

7.4.1A Minimum requirements for CA 192

7.4.1B Minimum requirements for UL-MIMO 193

7.4.1D Minimum requirements for ProSe 193

7.4A Void 194

7.4A.1 Void 194

7.5 Adjacent Channel Selectivity (ACS) 194

7.5.1 Minimum requirements 194

7.5.1A Minimum requirements for CA 195

7.5.1B Minimum requirements for UL-MIMO 197

7.5.1D Minimum requirements for ProSe 197

7.6 Blocking characteristics 198

7.6.1 In-band blocking 198

7.6.1.1 Minimum requirements 198

7.6.1.1A Minimum requirements for CA 199

7.6.1.1D Minimum requirements for ProSe 201

7.6.2 Out-of-band blocking 202

7.6.2.1 Minimum requirements 202

7.6.2.1A Minimum requirements for CA 203

7.6.2.1D Minimum requirements for ProSe 206

7.6.3 Narrow band blocking 206

7.6.3.1 Minimum requirements 207

7.6.3.1A Minimum requirements for CA 207

7.6.3.1D Minimum requirements for ProSe 208

7.6A Void 209

7.6B Blocking characteristics for UL-MIMO 209

7.7 Spurious response 209

7.7.1 Minimum requirements 209

7.7.1A Minimum requirements for CA 210

7.7.1B Minimum requirements for UL-MIMO 211

7.7.1D Minimum requirements for ProSe 211

7.8 Intermodulation characteristics 212

7.8.1 Wide band intermodulation 212

7.8.1.1 Minimum requirements 212

7.8.1A Minimum requirements for CA 212

7.8.1B Minimum requirements for UL-MIMO 214

7.8.1D Minimum requirements for ProSe 214

7.8.2 Void 215

7.9 Spurious emissions 215

7.9.1 Minimum requirements 215

7.9.1A Minimum requirements 215

7.10 Receiver image 215

7.10.1 Void 215

7.10.1A Minimum requirements for CA 215

8 Performance requirement 217

8.1 General 217

8.1.1 Receiver antenna capability 217

8.1.1.1 Simultaneous unicast and MBMS operations 218

8.1.1.2 Dual-antenna receiver capability in idle mode 218

8.1.2 Applicability of requirements 218

8.1.2.1 Applicability of requirements for different channel bandwidths 218

8.1.2.2 Definition of CA capability 218

8.1.2.2A Definition of dual connectivity capability 219

8.1.2.3 Applicability and test rules for different CA configurations and bandwidth combination sets 220

8.1.2.3A Applicability and test rules for different dual connectivity configuration and bandwidth combination set 222

8.1.2.3B Applicability and test rules for different TDD-FDD CA configurations and bandwidth combination sets 223

8.1.2.4 Test coverage for different number of component carriers 224

8.1.2.5 Applicability of performance requirements for Type B receiver 225

8.1.3 UE category and UE DL category 225

8.2 Demodulation of PDSCH (Cell-Specific Reference Symbols) 225

8.2.1 FDD (Fixed Reference Channel) 225

8.2.1.1 Single-antenna port performance 225

8.2.1.1.1 Minimum Requirement 226

8.2.1.1.2 Void 229

8.2.1.1.3 Void 229

8.2.1.1.4 Minimum Requirement 1 PRB allocation in presence of MBSFN 229

8.2.1.2 Transmit diversity performance 230

8.2.1.2.1 Minimum Requirement 2 Tx Antenna Port 230

8.2.1.2.2 Minimum Requirement 4 Tx Antenna Port 231

8.2.1.2.3 Minimum Requirement 2 Tx Antenna Port (demodulation subframe overlaps with aggressor cell ABS) 231

8.2.1.2.3A Minimum Requirement 2 Tx Antenna Ports (demodulation subframe overlaps with aggressor cell ABS and CRS assistance information are configured) 233

8.2.1.2.4 Enhanced Performance Requirement Type A - 2 Tx Antenna Ports with TM3 interference model 235

8.2.1.2.5 Enhanced Performance Requirement Type B - 2 Tx Antenna Ports with TM2 interference model 237

8.2.1.2.6 Enhanced Performance Requirement Type B - 2 Tx Antenna Ports with TM9 interference model 238

8.2.1.3 Open-loop spatial multiplexing performance 239

8.2.1.3.1 Minimum Requirement 2 Tx Antenna Port 239

8.2.1.3.1B Enhanced Performance Requirement Type C –2Tx Antenna Ports 242

8.2.1.3.1C Enhanced Performance Requirement Type C - 2 Tx Antenna Ports with TM1 interference 243

8.2.1.3.2 Minimum Requirement 4 Tx Antenna Port 244

8.2.1.3.3 Minimum Requirement 2 Tx Antenna Port (demodulation subframe overlaps with aggressor cell ABS) 244

8.2.1.3.4 Minimum Requirement 2 Tx Antenna Port (demodulation subframe overlaps with aggressor cell ABS and CRS assistance information are configured) 248

8.2.1.4 Closed-loop spatial multiplexing performance 250

8.2.1.4.1 Minimum Requirement Single-Layer Spatial Multiplexing 2 Tx Antenna Port 250

8.2.1.4.1A Minimum Requirement Single-Layer Spatial Multiplexing 4 Tx Antenna Port 251

8.2.1.4.1B Enhanced Performance Requirement Type A - Single-Layer Spatial Multiplexing 2 Tx Antenna Port with TM4 interference model 251

8.2.1.4.1C Minimum Requirement Single-Layer Spatial Multiplexing 2 Tx Antenna Ports (demodulation subframe overlaps with aggressor cell ABS and CRS assistance information are configured) 253

8.2.1.4.1D Enhanced Performance Requirement Type B - Single-layer Spatial Multiplexing 2 Tx Antenna Port with TM4 interference model 256

8.2.1.4.2 Minimum Requirement Multi-Layer Spatial Multiplexing 2 Tx Antenna Port 258

8.2.1.4.2A Enhanced Performance Requirement Type C – Multi-layer Spatial Multiplexing 2Tx Antenna Ports 258

8.2.1.4.3 Minimum Requirement Multi-Layer Spatial Multiplexing 4 Tx Antenna Port 259

8.2.1.4.3A Minimum Requirement Multi-Layer Spatial Multiplexing 4 Tx Antenna Port for dual connectivity 262

8.2.1.5 MU-MIMO 264

8.2.1.6 [Control channel performance: D-BCH and PCH] 264

8.2.1.7 Carrier aggregation with power imbalance 264

8.2.1.7.1 Minimum Requirement 264

8.2.1.8 Intra-band non-contiguous carrier aggregation with timing offset 265

8.2.1.8.1 Minimum Requirement 265

8.2.2 TDD (Fixed Reference Channel) 266

8.2.2.1 Single-antenna port performance 266

8.2.2.1.1 Minimum Requirement 266

8.2.2.1.2 Void 270

8.2.2.1.3 Void 270

8.2.2.1.4 Minimum Requirement 1 PRB allocation in presence of MBSFN 270

8.2.2.2 Transmit diversity performance 271

8.2.2.2.1 Minimum Requirement 2 Tx Antenna Port 271

8.2.2.2.2 Minimum Requirement 4 Tx Antenna Port 271

8.2.2.2.3 Minimum Requirement 2 Tx Antenna Port (demodulation subframe overlaps with aggressor cell ABS) 272

8.2.2.2.3A Minimum Requirement 2 Tx Antenna Ports (demodulation subframe overlaps with aggressor cell ABS and CRS assistance information are configured) 274

8.2.2.2.4 Enhanced Performance Requirement Type A – 2 Tx Antenna Ports with TM3 interference model 276

8.2.2.2.5 Minimum Requirement 2 Tx Antenna Port (when *EIMTA-MainConfigServCell-r12* is configured) 278

8.2.2.2.6 Enhanced Performance Requirement Type B - 2 Tx Antenna Ports with TM2 interference model 278

8.2.2.2.7 Enhanced Performance Requirement Type B - 2 Tx Antenna Ports with TM9 interference model 280

8.2.2.3 Open-loop spatial multiplexing performance 281

8.2.2.3.1 Minimum Requirement 2 Tx Antenna Port 281

8.2.2.3.1A Soft buffer management test 283

8.2.2.3.1B Enhanced Performance Requirement Type C - 2Tx Antenna Ports 284

8.2.2.3.1C Enhanced Performance Requirement Type C - 2 Tx Antenna Ports with TM1 interference 284

8.2.2.3.2 Minimum Requirement 4 Tx Antenna Port 285

8.2.2.3.3 Minimum Requirement 2Tx antenna port (demodulation subframe overlaps with aggressor cell ABS) 286

8.2.2.3.4 Minimum Requirement 2 Tx Antenna Port (demodulation subframe overlaps with aggressor cell ABS and CRS assistance information are configured) 290

8.2.2.4 Closed-loop spatial multiplexing performance 292

8.2.2.4.1 Minimum Requirement Single-Layer Spatial Multiplexing 2 Tx Antenna Port 292

8.2.2.4.1A Minimum Requirement Single-Layer Spatial Multiplexing 4 Tx Antenna Port 293

8.2.2.4.1B Enhanced Performance Requirement Type A – Single-Layer Spatial Multiplexing 2 Tx Antenna Port with TM4 interference model 293

8.2.2.4.1C Minimum Requirement Single-Layer Spatial Multiplexing 2 Tx Antenna Ports (demodulation subframe overlaps with aggressor cell ABS and CRS assistance information are configured) 295

8.2.2.4.1D Enhanced Performance Requirement Type B - Single-layer Spatial Multiplexing 2 Tx Antenna Port with TM4 interference model 297

8.2.2.4.2 Minimum Requirement Multi-Layer Spatial Multiplexing 2 Tx Antenna Port 299

8.2.2.4.2A Enhanced Performance Requirement Type C Multi-Layer Spatial Multiplexing 2 Tx Antenna Port 300

8.2.2.4.3 Minimum Requirement Multi-Layer Spatial Multiplexing 4 Tx Antenna Port 300

8.2.2.4.3A Minimum Requirement Multi-Layer Spatial Multiplexing 4 Tx Antenna Port for dual connectivity 303

8.2.2.4.4 Void 305

8.2.2.5 MU-MIMO 305

8.2.2.6 [Control channel performance: D-BCH and PCH] 305

8.2.2.7 Carrier aggregation with power imbalance 305

8.2.2.7.1 Minimum Requirement 305

8.2.2.8 Intra-band contiguous carrier aggregation with minimum channel spacing 306

8.2.2.8.1 Minimum Requirement 306

8.2.3 TDD FDD CA (Fixed Reference Channel) 307

8.2.3.1 Single-antenna port performance 308

8.2.3.1.1 Minimum Requirement for FDD PCell 308

8.2.3.1.2 Minimum Requirement for TDD PCell 310

8.2.3.2 Open-loop spatial multiplexing performance 2Tx Antenna port 312

8.2.3.2.1 Minimum Requirement for FDD PCell 312

8.2.3.2.1A Soft buffer management test for FDD PCell 314

8.2.3.2.2 Minimum Requirement for TDD PCell 315

8.2.3.2.2A Soft buffer management test for TDD PCell 317

8.2.3.3 Closed-loop spatial multiplexing performance 4Tx Antenna Port 318

8.2.3.3.1 Minimum Requirement for FDD PCell 318

8.2.3.3.2 Minimum Requirement for TDD PCell 320

8.3 Demodulation of PDSCH (User-Specific Reference Symbols) 322

8.3.1 FDD 322

8.3.1.1 Single-layer Spatial Multiplexing 323

8.3.1.1A Enhanced Performance Requirement Type A – Single-layer Spatial Multiplexing with TM9 interference model 325

8.3.1.1B Single-layer Spatial Multiplexing (demodulation subframe overlaps with aggressor cell ABS and CRS assistance information are configured) 328

8.3.1.1C Enhanced Performance Requirement Type B – Single-layer Spatial Multiplexing with TM9 interference model 331

8.3.1.1D Enhanced Performance Requirement Type B – Single-layer Spatial Multiplexing with CRS interference model 333

8.3.1.1E Enhanced Performance Requirement Type B – Single-layer Spatial Multiplexing with TM3 interference model 334

8.3.1.1F Enhanced Performance Requirement Type B – Single-layer Spatial Multiplexing with TM10 serving cell configuration and TM9 interference model 335

8.3.1.2 Dual-Layer Spatial Multiplexing 337

8.3.1.2A Enhanced Performance Requirement Type C - Dual-Layer Spatial Multiplexing 338

8.3.1.3 Performance requirements for DCI format 2D and non Quasi Co-located Antenna Ports 339

8.3.1.3.1 Minimum requirement with Same Cell ID (with single NZP CSI-RS resource) 339

8.3.1.3.2 Minimum requirements with Same Cell ID (with multiple NZP CSI-RS resources) 341

8.3.1.3.3 Minimum requirement with Different Cell ID and Colliding CRS (with single NZP CSI-RS resource) 343

8.3.2 TDD 345

8.3.2.1 Single-layer Spatial Multiplexing 345

8.3.2.1A Single-layer Spatial Multiplexing (with multiple CSI-RS configurations) 347

8.3.2.1B Enhanced Performance Requirement Type A – Single-layer Spatial Multiplexing with TM9 interference model 349

8.3.2.1C Single-layer Spatial Multiplexing (demodulation subframe overlaps with aggressor cell ABS and CRS assistance information are configured) 352

8.3.2.1D Enhanced Performance Requirement Type B – Single-layer Spatial Multiplexing with TM9 interference 355

8.3.2.1E Enhanced Performance Requirement Type B – Single-layer Spatial Multiplexing with CRS interference model 357

8.3.2.1F Enhanced Performance Requirement Type B – Single-layer Spatial Multiplexing with TM3 interference 359

8.3.2.1G Enhanced Performance Requirement Type B – Single-layer Spatial Multiplexing with TM10 serving cell configuration and TM9 interference model 360

8.3.2.2 Dual-Layer Spatial Multiplexing 362

8.3.2.2A Enhanced Performance Requirement Type C - Dual-Layer Spatial Multiplexing 363

8.3.2.3 Dual-Layer Spatial Multiplexing (with multiple CSI-RS configurations) 364

8.3.2.4 Performance requirements for DCI format 2D and non Quasi Co-located Antenna Ports 365

8.3.2.4.1 Minimum requirement with Same Cell ID (with single NZP CSI-RS resource) 365

8.3.2.4.2 Minimum requirements with Same Cell ID (with multiple NZP CSI-RS resources) 367

8.3.2.4.3 Minimum requirement with Different Cell ID and Colliding CRS (with single NZP CSI-RS resource) 369

8.4 Demodulation of PDCCH/PCFICH 371

8.4.1 FDD 371

8.4.1.1 Single-antenna port performance 371

8.4.1.2 Transmit diversity performance 371

8.4.1.2.1 Minimum Requirement 2 Tx Antenna Port 371

8.4.1.2.2 Minimum Requirement 4 Tx Antenna Port 372

8.4.1.2.3 Minimum Requirement 2 Tx Antenna Port (demodulation subframe overlaps with aggressor cell ABS) 372

8.4.1.2.4 Minimum Requirement 2 Tx Antenna Port (demodulation subframe overlaps with aggressor cell ABS and CRS assistance information are configured) 377

8.4.2 TDD 382

8.4.2.1 Single-antenna port performance 383

8.4.2.2 Transmit diversity performance 383

8.4.2.2.1 Minimum Requirement 2 Tx Antenna Port 383

8.4.2.2.2 Minimum Requirement 4 Tx Antenna Port 384

8.4.2.2.3 Minimum Requirement 2 Tx Antenna Port (demodulation subframe overlaps with aggressor cell ABS) 384

8.4.2.2.4 Minimum Requirement 2 Tx Antenna Port (demodulation subframe overlaps with aggressor cell ABS and CRS assistance information are configured) 388

8.5 Demodulation of PHICH 392

8.5.1 FDD 392

8.5.1.1 Single-antenna port performance 392

8.5.1.2 Transmit diversity performance 393

8.5.1.2.1 Minimum Requirement 2 Tx Antenna Port 393

8.5.1.2.2 Minimum Requirement 4 Tx Antenna Port 393

8.5.1.2.3 Minimum Requirement 2 Tx Antenna Port (demodulation subframe overlaps with aggressor cell ABS) 393

8.5.1.2.4 Minimum Requirement 2 Tx Antenna Port (demodulation subframe overlaps with aggressor cell ABS and CRS assistance information are configured) 395

8.5.2 TDD 398

8.5.2.1 Single-antenna port performance 399

8.5.2.2 Transmit diversity performance 399

8.5.2.2.1 Minimum Requirement 2 Tx Antenna Port 399

8.5.2.2.2 Minimum Requirement 4 Tx Antenna Port 400

8.5.2.2.3 Minimum Requirement 2 Tx Antenna Port (demodulation subframe overlaps with aggressor cell ABS) 400

8.5.2.2.4 Minimum Requirement 2 Tx Antenna Port (demodulation subframe overlaps with aggressor cell ABS and CRS assistance information are configured) 402

8.6 Demodulation of PBCH 404

8.6.1 FDD 404

8.6.1.1 Single-antenna port performance 404

8.6.1.2 Transmit diversity performance 404

8.6.1.2.1 Minimum Requirement 2 Tx Antenna Port 404

8.6.1.2.2 Minimum Requirement 4 Tx Antenna Port 405

8.6.1.2.3 Minimum Requirement 2 Tx Antenna Port under Time Domain Measurement Resource Restriction with CRS Assistance Information 405

8.6.2 TDD 407

8.6.2.1 Single-antenna port performance 407

8.6.2.2 Transmit diversity performance 407

8.6.2.2.1 Minimum Requirement 2 Tx Antenna Port 407

8.6.2.2.2 Minimum Requirement 4 Tx Antenna Port 407

8.6.2.2.3 Minimum Requirement 2 Tx Antenna Port under Time Domain Measurement Resource Restriction with CRS Assistance Information 408

8.7 Sustained downlink data rate provided by lower layers 409

8.7.1 FDD (single carrier and CA) 409

8.7.2 TDD (single carrier and CA) 414

8.7.3 FDD (EPDCCH scheduling) 417

8.7.4 TDD (EPDCCH scheduling) 418

8.7.5 TDD FDD CA 420

8.7.5.1 Minimum Requirement FDD PCell 421

8.7.5.2 Minimum Requirement TDD PCell 423

8.7.6 FDD (DC) 424

8.7.7 TDD (DC) 427

8.8 Demodulation of EPDCCH 430

8.8.1 Distributed Transmission 430

8.8.1.1 FDD 430

8.8.1.1.1 Void 431

8.8.1.2 TDD 431

8.8.1.2.1 Void 432

8.8.2 Localized Transmission with TM9 432

8.8.2.1 FDD 432

8.8.2.1.1 Void 433

8.8.2.1.2 Void 433

8.8.2.2 TDD 433

8.8.2.2.1 Void 434

8.8.2.2.2 Void 434

8.8.3 Localized transmission with TM10 Type B quasi co-location type 435

8.8.3.1 FDD 435

8.8.3.2 TDD 438

8.9 Demodulation (single receiver antenna) 441

8.9.1 PDSCH 441

8.9.1.1 FDD and half-duplex FDD (Fixed Reference Channel) 441

8.9.1.1.1 Transmit diversity performance (Cell-Specific Reference Symbols) 442

8.9.1.1.2 Closed-loop spatial multiplexing performance (Cell-Specific Reference Symbols) 442

8.9.1.1.3 Closed-loop spatial multiplexing performance (User-Specific Reference Symbols) 443

8.9.1.2 TDD (Fixed Reference Channel) 444

8.9.1.2.1 Transmit diversity performance (Cell-Specific Reference Symbols) 445

8.9.1.2.2 Closed-loop spatial multiplexing performance (Cell-Specific Reference Symbols) 446

8.9.1.2.3 Closed-loop spatial multiplexing performance (User-Specific Reference Symbols) 446

8.9.2 PHICH 448

8.9.2.1 FDD and half-duplex FDD 448

8.9.2.1.1 Transmit diversity performance 448

8.9.2.2 TDD 448

8.9.2.2.1 Transmit diversity performance 448

8.9.3 PBCH 448

8.9.3.1 FDD and half-duplex FDD 448

8.9.3.1.1 Transmit diversity performance 448

8.9.3.2 TDD 449

8.9.3.2.1 Transmit diversity performance 449

9 Reporting of Channel State Information 449

9.1 General 449

9.1.1 Applicability of requirements 449

9.1.1.1 Applicability of requirements for different channel bandwidths 449

9.1.1.2 Applicability and test rules for different CA configurations and bandwidth combination sets 449

9.1.1.2A Applicability and test rules for different TDD-FDD CA configurations and bandwidth combination sets 450

9.1.1.3 Test coverage for different number of componenet carriers 451

9.2 CQI reporting definition under AWGN conditions 451

9.2.1 Minimum requirement PUCCH 1-0 (Cell-Specific Reference Symbols) 452

9.2.1.1 FDD 452

9.2.1.2 TDD 453

9.2.1.3 FDD (CSI measurements in case two CSI subframe sets are configured) 454

9.2.1.4 TDD (CSI measurements in case two CSI subframe sets are configured) 457

9.2.1.5 FDD (CSI measurements in case two CSI subframe sets are configured and with CRS assistance information) 460

9.2.1.6 TDD (CSI measurements in case two CSI subframe sets are configured and with CRS assistance information) 463

9.2.1.7 FDD (Modulation and TBS index Table 2 and 4-bit CQI Table 2 are used) 466

9.2.1.8 TDD (Modulation and TBS index Table 2 and 4-bit CQI Table 2 are used) 467

9.2.2 Minimum requirement PUCCH 1-1 (Cell-Specific Reference Symbols) 467

9.2.2.1 FDD 467

9.2.2.2 TDD 468

9.2.3 Minimum requirement PUCCH 1-1 (CSI Reference Symbols) 469

9.2.3.1 FDD 469

9.2.3.2 TDD 470

9.2.4 Minimum requirement PUCCH 1-1 (With Single CSI Process) 471

9.2.4.1 FDD 471

9.2.4.2 TDD 474

9.2.5 Minimum requirement PUCCH 1-1 (when *csi-SubframeSet –r12* and *EIMTA-MainConfigServCell-r12* are configured) 477

9.3 CQI reporting under fading conditions 480

9.3.1 Frequency-selective scheduling mode 480

9.3.1.1 Minimum requirement PUSCH 3-0 (Cell-Specific Reference Symbols) 480

9.3.1.1.1 FDD 480

9.3.1.1.2 TDD 481

9.3.1.1.3 FDD (CSI measurements in case two CSI subframe sets are configured and with CRS assistance information) 482

9.3.1.1.4 TDD (CSI measurements in case two CSI subframe sets are configured and with CRS assistance information) 486

9.3.1.1.5 TDD (when *csi-SubframeSet –r12* is configured) 489

9.3.1.2 Minimum requirement PUSCH 3-1 (CSI Reference Symbol) 491

9.3.1.2.1 FDD 491

9.3.1.2.2 TDD 492

9.3.1.2.3 FDD (Modulation and TBS index Table 2 and 4-bit CQI Table 2 are used) 494

9.3.1.2.4 TDD (Modulation and TBS index Table 2 and 4-bit CQI Table 2 are used) 495

9.3.1.2.5 Void 496

9.3.1.2.6 TDD (when *csi-SubframeSet –r12* is configured with one CSI process) 496

9.3.2 Frequency non-selective scheduling mode 500

9.3.2.1 Minimum requirement PUCCH 1-0 (Cell-Specific Reference Symbol) 500

9.3.2.1.1 FDD 500

9.3.2.1.2 TDD 502

9.3.2.2 Minimum requirement PUCCH 1-1 (CSI Reference Symbol) 504

9.3.2.2.1 FDD 504

9.3.2.2.2 TDD 505

9.3.3 Frequency-selective interference 507

9.3.3.1 Minimum requirement PUSCH 3-0 (Cell-Specific Reference Symbol) 507

9.3.3.1.1 FDD 507

9.3.3.1.2 TDD 508

9.3.3.2 Void 509

9.3.3.2.1 Void 509

9.3.3.2.2 Void 509

9.3.4 UE-selected subband CQI 509

9.3.4.1 Minimum requirement PUSCH 2-0 (Cell-Specific Reference Symbols) 509

9.3.4.1.1 FDD 509

9.3.4.1.2 TDD 510

9.3.4.2 Minimum requirement PUCCH 2-0 (Cell-Specific Reference Symbols) 511

9.3.4.2.1 FDD 511

9.3.4.2.2 TDD 513

9.3.5 Additional requirements for enhanced receiver Type A 515

9.3.5.1 Minimum requirement PUCCH 1-0 (Cell-Specific Reference Symbol) 515

9.3.5.1.1 FDD 515

9.3.5.1.2 TDD 516

9.3.5.2 Minimum requirement PUCCH 1-1 (CSI Reference Symbol) 519

9.3.5.2.1 FDD 519

9.3.5.2.2 TDD 522

9.3.6 Minimum requirement (With multiple CSI processes) 525

9.3.6.1 FDD 525

9.3.6.2 TDD 530

9.3.7 Minimum requirement PUSCH 3-2 534

9.3.7.1 FDD 534

9.3.7.2 TDD 535

9.3.8 Additional requirements for enhanced receiver Type B 537

9.3.8.1 Minimum requirement PUCCH 1-1 (Cell-Specific Reference Symbols) 537

9.3.8.1.1 FDD 537

9.3.8.1.2 TDD 538

9.3.8.2 Minimum requirement PUCCH 1-1 (CSI Reference Symbols) 540

9.3.8.2.1 FDD 540

9.3.8.2.2 TDD 542

9.3.8.3 Minimum requirement with CSI process 545

9.3.8.3.1 FDD 545

9.3.8.3.2 TDD 548

9.4 Reporting of Precoding Matrix Indicator (PMI) 551

9.4.1 Single PMI 552

9.4.1.1 Minimum requirement PUSCH 3-1 (Cell-Specific Reference Symbols) 552

9.4.1.1.1 FDD 552

9.4.1.1.2 TDD 552

9.4.1.2 Minimum requirement PUCCH 2-1 (Cell-Specific Reference Symbols) 553

9.4.1.2.1 FDD 553

9.4.1.2.2 TDD 555

9.4.1.3 Minimum requirement PUSCH 3-1 (CSI Reference Symbol) 556

9.4.1.3.1 FDD 556

9.4.1.3.2 TDD 557

9.4.1.4 Minimum requirement PUCCH 1-1 (CSI Reference Symbol) 560

9.4.1.4.1 FDD (with 4Tx enhanced codebook) 560

9.4.1.4.2 TDD (with 4Tx enhanced codebook) 562

9.4.1a Void 565

9.4.1a.1 Void 565

9.4.1a.1.1 Void 565

9.4.1a.1.2 Void 565

9.4.2 Multiple PMI 565

9.4.2.1 Minimum requirement PUSCH 1-2 (Cell-Specific Reference Symbols) 565

9.4.2.1.1 FDD 565

9.4.2.1.2 TDD 566

9.4.2.2 Minimum requirement PUSCH 2-2 (Cell-Specific Reference Symbols) 567

9.4.2.2.1 FDD 567

9.4.2.2.2 TDD 568

9.4.2.3 Minimum requirement PUSCH 1-2 (CSI Reference Symbol) 569

9.4.2.3.1 FDD 569

9.4.2.3.2 TDD 571

9.4.2.3.3 FDD (with 4Tx enhanced codebook) 574

9.4.2.3.4 TDD (with 4Tx enhanced codebook) 576

9.4.3 Void 578

9.4.3.1 Void 578

9.4.3.1.1 Void 578

9.4.3.1.2 Void 578

9.5 Reporting of Rank Indicator (RI) 578

9.5.1 Minimum requirement (Cell-Specific Reference Symbols) 578

9.5.1.1 FDD 578

9.5.1.2 TDD 579

9.5.2 Minimum requirement (CSI Reference Symbols) 580

9.5.2.1 FDD 580

9.5.2.2 TDD 582

9.5.3 Minimum requirement (CSI measurements in case two CSI subframe sets are configured) 584

9.5.3.1 FDD 584

9.5.3.2 TDD 587

9.5.4 Minimum requirement (CSI measurements in case two CSI subframe sets are configured and CRS assistance information are configured) 590

9.5.4.1 FDD 590

9.5.4.2 TDD 593

9.5.5 Minimum requirement (with CSI process) 596

9.5.5.1 FDD 597

9.5.5.2 TDD 600

9.6 Additional requirements for carrier aggregation 603

9.6.1 Periodic reporting on multiple cells (Cell-Specific Reference Symbols) 603

9.6.1.1 FDD 603

9.6.1.2 TDD 605

9.6.1.3 TDD-FDD CA with FDD PCell 607

9.6.1.4 TDD-FDD CA with TDD PCell 609

9.7 CSI reporting (Single receiver antenna) 611

9.7.1 CQI reporting definition under AWGN conditions 611

9.7.1.1 FDD and half-duplex FDD 611

9.7.1.2 TDD 612

9.7.2 CQI reporting under fading conditions 613

9.7.2.1 FDD and half-duplex FDD 613

9.7.2.2 TDD 614

10 Performance requirement (MBMS) 615

10.1 FDD (Fixed Reference Channel) 615

10.1.1 Minimum requirement 616

10.2 TDD (Fixed Reference Channel) 616

10.2.1 Minimum requirement 617

11 Performance requirement (ProSe Direct Discovery) 617

11.1 General 618

11.1.1 Applicability of requirements 618

11.1.2 Reference DRX configuration 618

11.2 Demodulation of PSDCH (single link performance) 618

11.2.1 FDD 618

11.2.2 TDD 619

11.3 Power imbalance performance with two links 620

11.3.1 FDD 620

11.3.2 TDD 621

11.4 Multiple timing reference test 622

11.4.1 FDD 623

11.5 Maximum Sidelink processes test 624

11.5.1 FDD 624

11.5.2 TDD 625

12 Performance requirement (ProSe Direct Communication) 627

12.1 General 627

12.1.1 Applicability of requirements 627

12.1.2 Reference DRX configuration 627

12.2 Demodulation of PSSCH 627

12.2.1 FDD 627

12.3 Demodulation of PSCCH 628

12.3.1 FDD 629

12.4 Demodulation of PSBCH 630

12.4.1 FDD 630

12.5 Power imbalance performance with two links 630

12.5.1 FDD 630

12.6 Multiple timing reference test 632

12.6.1 FDD 632

12.7 Maximum Sidelink processes test 635

12.7.1 FDD 635

12.8 Sustained downlink data rate with active Sidelink 636

Annex A (normative): Measurement channels 639

A.1 General 639

A.2 UL reference measurement channels 639

A.2.1 General 639

A.2.1.1 Applicability and common parameters 639

A.2.1.2 Determination of payload size 639

A.2.1.3 Overview of UL reference measurement channels 640

A.2.2 Reference measurement channels for FDD 649

A.2.2.1 Full RB allocation 649

A.2.2.1.1 QPSK 649

A.2.2.1.2 16-QAM 650

A.2.2.1.3 64-QAM 650

A.2.2.2 Partial RB allocation 650

A.2.2.2.1 QPSK 651

A.2.2.2.2 16-QAM 653

A.2.2.2.3 64-QAM 653

A.2.2.3 Void 654

A.2.3 Reference measurement channels for TDD 654

A.2.3.1 Full RB allocation 654

A.2.3.1.1 QPSK 654

A.2.3.1.2 16-QAM 655

A.2.3.1.3 64-QAM 656

A.2.3.2 Partial RB allocation 656

A.2.3.2.1 QPSK 657

A.2.3.2.2 16-QAM 659

A.2.3.2.3 64-QAM 660

A.2.3.3 Void 660

A.3 DL reference measurement channels 660

A.3.1 General 660

A.3.1.1 Overview of DL reference measurement channels 660

A.3.2 Reference measurement channel for receiver characteristics 674

A.3.3 Reference measurement channels for PDSCH performance requirements (FDD) 687

A.3.3.1 Single-antenna transmission (Common Reference Symbols) 687

A.3.3.2 Multi-antenna transmission (Common Reference Symbols) 692

A.3.3.2.1 Two antenna ports 692

A.3.3.2.2 Four antenna ports 694

A.3.3.3 Reference Measurement Channel for UE-Specific Reference Symbols 694

A.3.3.3.0 Two antenna ports (no CSI-RS) 694

A.3.3.3.1 Two antenna port (CSI-RS) 695

A.3.3.3.2 Four antenna ports (CSI-RS) 697

A.3.4 Reference measurement channels for PDSCH performance requirements (TDD) 702

A.3.4.1 Single-antenna transmission (Common Reference Symbols) 702

A.3.4.2 Multi-antenna transmission (Common Reference Signals) 710

A.3.4.2.1 Two antenna ports 710

A.3.4.2.2 Four antenna ports 715

A.3.4.3 Reference Measurement Channels for UE-Specific Reference Symbols 716

A.3.4.3.1 Single antenna port (Cell Specific) 716

A.3.4.3.2 Two antenna ports (Cell Specific) 716

A.3.4.3.3 Two antenna ports (CSI-RS) 718

A.3.4.3.4 Four antenna ports (CSI-RS) 720

A.3.4.3.5 Eight antenna ports (CSI-RS) 724

A.3.5 Reference measurement channels for PDCCH/PCFICH performance requirements 727

A.3.5.1 FDD 727

A.3.5.2 TDD 727

A.3.6 Reference measurement channels for PHICH performance requirements 727

A.3.7 Reference measurement channels for PBCH performance requirements 728

A.3.8 Reference measurement channels for MBMS performance requirements 728

A.3.8.1 FDD 728

A.3.8.2 TDD 730

A.3.9 Reference measurement channels for sustained downlink data rate provided by lower layers 732

A.3.9.1 FDD 732

A.3.9.2 TDD 735

A.3.9.3 FDD (EPDCCH scheduling) 740

A.3.9.4 TDD (EPDCCH scheduling) 741

A.3.10 Reference Measurement Channels for EPDCCH performance requirements 742

A.3.10.1 FDD 742

A.3.10.2 TDD 743

A.4 CSI reference measurement channels 743

A.5 OFDMA Channel Noise Generator (OCNG) 754

A.5.1 OCNG Patterns for FDD 754

A.5.1.1 OCNG FDD pattern 1: One sided dynamic OCNG FDD pattern 754

A.5.1.2 OCNG FDD pattern 2: Two sided dynamic OCNG FDD pattern 755

A.5.1.3 OCNG FDD pattern 3: 49 RB OCNG allocation with MBSFN in 10 MHz 755

A.5.1.4 OCNG FDD pattern 4: One sided dynamic OCNG FDD pattern for MBMS transmission 756

A.5.1.5 OCNG FDD pattern 5: One sided dynamic 16QAM modulated OCNG FDD pattern 756

A.5.1.6 OCNG FDD pattern 6: dynamic OCNG FDD pattern when user data is in 2 non-contiguous blocks 757

A.5.1.8 OCNG FDD pattern 8: Dynamic OCNG FDD pattern for TM10 transmission 758

A.5.2 OCNG Patterns for TDD 759

A.5.2.1 OCNG TDD pattern 1: One sided dynamic OCNG TDD pattern 759

A.5.2.2 OCNG TDD pattern 2: Two sided dynamic OCNG TDD pattern 760

A.5.2.3 OCNG TDD pattern 3: 49 RB OCNG allocation with MBSFN in 10 MHz 761

A.5.2.4 OCNG TDD pattern 4: One sided dynamic OCNG TDD pattern for MBMS transmission 761

A.5.2.5 OCNG TDD pattern 5: One sided dynamic 16QAM modulated OCNG TDD pattern 762

A.5.2.6 OCNG TDD pattern 6: dynamic OCNG TDD pattern when user data is in 2 non-contiguous blocks 763

A.5.2.8 OCNG TDD pattern 8: Dynamic OCNG TDD pattern for TM10 transmission 764

A.6 Sidelink reference measurement channels 765

A.6.1 General 765

A.6.1.1 Overview of ProSe reference measurement channels 765

A.6.2 Reference measurement channel for receiver characteristics 766

A.6.4 Reference measurement channels for PSCCH performance requirements 769

A.6.5 Reference measurement channels for PSSCH performance requirements 770

A.6.6 Reference measurement channels for PSBCH performance requirements 770

A.7 Sidelink reference resource pool configurations 771

A.7.1 Reference resource pool configurations for ProSe Direct Discovery demodulation tests 771

A.7.1.1 FDD 771

A.7.1.2 TDD 773

A.7.2 Reference resource pool configurations for ProSe Direct Communication demodulation tests 775

A.7.2.1 FDD 775

Annex B (normative): Propagation conditions 781

B.1 Static propagation condition 781

B.2 Multi-path fading propagation conditions 781

B.2.1 Delay profiles 781

B.2.2 Combinations of channel model parameters 782

B.2.3 MIMO Channel Correlation Matrices 783

B.2.3.1 Definition of MIMO Correlation Matrices 783

B.2.3.2 MIMO Correlation Matrices at High, Medium and Low Level 784

B.2.3A MIMO Channel Correlation Matrices using cross polarized antennas 786

B.2.3A.1 Definition of MIMO Correlation Matrices using cross polarized antennas 787

B.2.3A.2 Spatial Correlation Matrices using cross polarized antennas at eNB and UE sides 787

B.2.3A.2.1 Spatial Correlation Matrices at eNB side 787

B.2.3A.2.2 Spatial Correlation Matrices at UE side 788

B.2.3A.4 Beam steering approach 789

B.2.4 Propagation conditions for CQI tests 789

B.2.4.1 Propagation conditions for CQI tests with multiple CSI processes 789

B.2.5 Void 790

B.2.6 MBSFN Propagation Channel Profile 790

B.3 High speed train scenario 790

B.4 Beamforming Model 792

B.4.1 Single-layer random beamforming (Antenna port 5, 7, or 8) 792

B.4.2 Dual-layer random beamforming (antenna ports 7 and 8) 792

B.4.3 Generic beamforming model (antenna ports 7-14) 793

B.4.4 Random beamforming for EPDCCH distributed transmission (Antenna port 107 and 109) 793

B.4.5 Random beamforming for EPDCCH localized transmission (Antenna port 107, 108, 109 or 110) 794

B.5 Interference models for enhanced performance requirements Type-A 794

B.5.1 Dominant interferer proportion 794

B.5.2 Transmission mode 3 interference model 794

B.5.3 Transmission mode 4 interference model 795

B.5.4 Transmission mode 9 interference model 795

B.6 Interference models for enhanced performance requirements Type-B 796

B.6.1 Transmission mode 2 interference model 796

B.6.2 Transmission mode 3 interference model 796

B.6.3 Transmission mode 4 interference model 796

B.6.4 Transmission mode 9 interference model 797

B.6.5 CRS interference model 797

B.6.6 Random interference model 797

Annex C (normative): Downlink Physical Channels 799

C.1 General 799

C.2 Set-up 799

C.3 Connection 799

C.3.1 Measurement of Receiver Characteristics 799

C.3.2 Measurement of Performance requirements 800

C.3.3 Aggressor cell power allocation for Measurement of Performance Requirements when ABS is Configured 801

C.3.4 Power Allocation for Measurement of Performance Requirements when Quasi Co-location Type B: same Cell ID 802

C.3.5 Simplified CA testing method 802

Annex D (normative): Characteristics of the interfering signal 804

D.1 General 804

D.2 Interference signals 804

Annex E (normative): Environmental conditions 805

E.1 General 805

E.2 Environmental 805

E.2.1 Temperature 805

E.2.2 Voltage 805

E.2.3 Vibration 806

Annex F (normative): Transmit modulation 807

F.1 Measurement Point 807

F.2 Basic Error Vector Magnitude measurement 807

F.3 Basic in-band emissions measurement 808

F.4 Modified signal under test 808

F.5 Window length 810

F.5.1 Timing offset 810

F.5.2 Window length 810

F.5.3 Window length for normal CP 810

F.5.4 Window length for Extended CP 811

F.5.5 Window length for PRACH 811

F.6 Averaged EVM 812

F.7 Spectrum Flatness 813

Annex G (informative): Reference sensitivity level in lower SNR 814

G.1 General 814

G.2 Typical receiver sensitivity performance (QPSK) 814

G.3 Reference measurement channel for REFSENSE in lower SNR 817

Annex H (normative): Modified MPR behavior 820

H.1 Indication of modified MPR behavior 820

Annex I (informative): Change history 821