3GPP TS 36.307 V12.17.0 (2018-06)

Technical Specification

3rd Generation Partnership Project;

Technical Specification Group Radio Access Network;

Evolved Universal Terrestrial Radio Access (E-UTRA);   
Requirements on User Equipments (UEs)

Supporting a release-independent frequency band

(Release 12)

 

The present document has been developed within the 3rd Generation Partnership Project (3GPP TM) and may be further elaborated for the purposes of 3GPP.  
The present document has not been subject to any approval process by the 3GPPOrganizational Partners and shall not be implemented.

This Specification is provided for future development work within 3GPPonly. The Organizational Partners accept no liability for any use of this Specification.  
Specifications and reports for implementation of the 3GPP TM system should be obtained via the 3GPP Organizational Partners' Publications Offices.

***3GPP***

Postal address

3GPP support office address

650 Route des Lucioles - Sophia Antipolis

Valbonne - FRANCE

Tel.: +33 4 92 94 42 00 Fax: +33 4 93 65 47 16

Internet

http://www.3gpp.org

***Copyright Notification***

No part may be reproduced except as authorized by written permission.  
The copyright and the foregoing restriction extend to reproduction in all media.

© 2018, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

All rights reserved.

UMTS™ is a Trade Mark of ETSI registered for the benefit of its members

3GPP™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners  
LTE™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners

GSM® and the GSM logo are registered and owned by the GSM Association

Contents

Foreword 4

1 Scope 5

2 References 5

3 Definitions and abbreviations 5

3.1 Definitions 5

3.2 Abbreviations 6

3.3 Symbols 6

3A Release independent features 6

3A.0 General 6

3A.1 Additional E-UTRA operating bands 6

3A.2 Additional E-UTRA CA configurations 7

3A.3 Additional operating bands and/or CA configurations for specific features 9

3A.4 Other release independent features 9

4 - 292 Void 10

Annex A (informative) : Frequency arrangement for overlapping operating bands 11

Annex B (normative): Common Requirements 12

B.1 Purpose of annex 12

B.2 Common RRM requirements 12

B.2.1 Common RRM requirements for a release independent band 12

B.2.2 Common RRM requirements for an intra-band contiguous CA configuration 13

B.2.3 Common RRM requirements for an intra-band non-contiguous CA with single uplink configuration 14

B.2.4 Common RRM requirements for an inter-band CA with single uplink configuration 15

B.2.5 Common RRM requirements for an inter-band CA with dual uplink configuration 15

B.2.6 Common RRM requirements for an intra-band non-contiguous CA with dual uplink configuration 16

B.2.7 Void 17

B.2.8 Void 17

B.2.9 Void 17

B.3 Common UE performance requirements 17

B.3.1 Void 17

B.3.2 Common UE performance requirements and tests for different CA configurations and combination sets 17

B.3.3 Void 18

B.3.4 Void 18

B.3.5 Void 18

B.4 Common UE RF requirements 18

B.4.1 Common UE RF requirements for a release independent band 18

B.4.2 Common UE RF requirements for an intra-band contiguous CA configuration 18

B.4.3 Common UE RF requirements for an single uplink inter-band CA configuration 19

B.4.4 Common UE RF requirements for an inter-band CA configuration including an operating band without uplink band 20

B.4.5 Common UE RF requirements for a single uplink intra-band non-contiguous CA configuration 20

B.4.6 Common UE RF requirements for a dual uplink inter-band CA configuration 21

B.4.7 Common UE RF requirements for a dual uplink intra-band non-contiguous CA configuration 21

B.4.8 Void 22

B.4.9 Void 22

B.4.10 Void 22

Annex C (informative): Change history 23

# Foreword

This Technical Specification has been produced by the 3rd Generation Partnership Project (3GPP).

The contents of the present document are subject to continuing work within the TSG and may change following formal TSG approval. Should the TSG modify the contents of the present document, it will be re-released by the TSG with an identifying change of release date and an increase in version number as follows:

Version x.y.z

where:

x the first digit:

1 presented to TSG for information;

2 presented to TSG for approval;

3 or greater indicates TSG approved document under change control.

y the second digit is incremented for all changes of substance, i.e. technical enhancements, corrections, updates, etc.

z the third digit is incremented when editorial only changes have been incorporated in the document.

# 1 Scope

The present document specifies requirements for Rel-12 UEs supporting release independent features like:

- additional E-UTRA operating frequency bands on top of Rel-12 of TS 36.101 [2] and TS 36.133 [3];

- additional E-UTRA CA configurations (intra-band/inter-band) on top of Rel-12 of TS 36.101 [2] and TS 36.133 [3];

- additional operating bands and/or CA configurations for specific features (like UE category 0);

- other release independent features (like 4Rx antenna port).

# 2 References

The following documents contain provisions which, through reference in this text, constitute provisions of the present document.

 References are either specific (identified by date of publication, edition number, version number, etc.) or non‑specific.

 For a specific reference, subsequent revisions do not apply.

 For a non-specific reference, the latest version applies. In the case of a reference to a 3GPP document (including a GSM document), a non-specific reference implicitly refers to the latest version of that document *in the same Release as the present document*.

[1] 3GPP TR 21.905: "Vocabulary for 3GPP Specifications".

[2] 3GPP TS 36.101: "Evolved Universal Terrestrial Radio Access (E-UTRA); User Equipment (UE) Radio Transmission and Reception".

NOTE: The considered release is given in the text of the present document that uses [2].

[3] 3GPP TS 36.133: "Evolved Universal Terrestrial Radio Access (E-UTRA); Requirements for Support of Radio Resource Management".

NOTE: The considered release is given in the text of the present document that uses [3].

[4] 3GPP TS 36.306: "Evolved Universal Terrestrial Radio Access (E-UTRA); User Equipment (UE) radio access capabilities".

NOTE: The considered release is given in the text of the present document that uses [4].

[5] Void.

# 3 Definitions and abbreviations

## 3.1 Definitions

For the purposes of the present document, the terms and definitions given in 3GPP TR 21.905 [1] and the following apply. A term defined in the present document takes precedence over the definition of the same term, if any, in 3GPP TR 21.905 [1].

**release independent**: applicable to some frozen releases, starting from a certain release Rel-M

NOTE 1: Normally, a feature is introduced only in the latest open release Rel-N and future releases are based on the previous one so that future releases inherit the requirements of this feature. Introducing a feature "in a release independent way from Rel-M onwards" (M<N) means it was decided by TSG RAN that this feature would be also beneficial in previous, already frozen releases starting with Rel-M until Rel-(N-1). In order to avoid touching TS 36.101 [2] or TS 36.133 [3] of these frozen releases, the corresponding requirements are captured in TS 36.307 via pointers to [2] or [3] of the release in which the feature was introduced.

NOTE 2: Release independent does not mean applicable to all releases.

## 3.2 Abbreviations

For the purposes of the present document, the abbreviations given in 3GPP TR 21.905 [1] and the following apply. An abbreviation defined in the present document takes precedence over the definition of the same abbreviation, if any, in 3GPP TR 21.905 [1].

4Rx 4 UE receiver antenna ports

CA Carrier Aggregation

CSI Channel State Indicator

FDD Frequency Division Duplex

RRC Radio Resource Control

RRM Radio Resource Management

TDD Time Division Duplex

UE User Equipment

## 3.3 Symbols

For the purposes of the present document, the following symbols apply:

N Release in which a feature is introduced into TS 36.101 [2] or TS 36.133 [3]

M Release from which onwards (including release M) a feature is release independent

# 3A Release independent features

## 3A.0 General

TSG-RAN has agreed for certain features (see the following clauses) to introduce them in a "release independent way".

This means for each feature:

- it is "introduced" in a release N, i.e. TS 36.101 [2] and TS 36.133 [3] of release N define certain UE requirements for this feature; the feature is indicated in the tables of the following clauses;

- it is "release independent" starting from a release M (M<N); M for the given feature is provided in the tables of the following clauses;

- UEs supporting this feature have to fulfill additional requirements in release M or higher which are specified in one or more Annexes of TS 36.307 of release N; the applicable Annexes for a given feature are provided in the tables of the following clauses.

The applicable UE Categories are specified in TS 36.306 [4] according to the release to which the UE conforms.

## 3A.1 Additional E-UTRA operating bands

Requirements for a Rel-12 UE for additional E-UTRA operating bands compared to TS 36.101 Rel-12 [2] are introduced via this clause.

Table 3A.1-1: E-UTRA operating bands and UE power class

|  |  |  |  |
| --- | --- | --- | --- |
| Feature | Duplex-mode | Release  independent from | Requirements to be fulfilled  (see TS 36.307 of the release in which the band was introduced) |
| Operating bands, band number <= 64, Power Class 3 | FDD, TDD | Rel-8 | Table B.2.1-1, Table B.4.1-1 |
| Operating bands, band number > 64, Power Class 3 | FDD, TDD | Rel-9 | Table B.2.1-1, Table B.4.1-1 |
| Operating bands, NS-value > 32 | FDD, TDD | Rel-10 | Table B.2.1-1, Table B.4.1-1 |
| Asymmetric operating bands, Power Class 3 | FDD | Rel-10 | Table B.2.1-1, Table B.4.1-1 |
| Operating bands, band number <= 64, Power Class 1 | FDD | Rel-10 | Table B.2.1-1, Table B.4.1-1 |
| Operating bands, Power Class 2 | TDD | Rel-10 | Table B.2.1-1, Table B.4.1-1 |

For example, Band 19 was introduced in the Release 9 specifications. In order to implement a UE conforming to Release 8 but supporting Band 19, it is necessary for the UE to additionally conform to some parts of the Release 9 specifications (see corresponding Annexes of TS 36.307 Rel-9 which will point to the requirements in the Rel-9 of TS 36.101 [2] or TS 36.133 [3] to be fulfilled), such as the radio frequency and radio resource management requirements for the Band 19.

## 3A.2 Additional E-UTRA CA configurations

Requirements for a Rel-12 UE for additional E-UTRA CA configurations compared to TS 36.101 Rel-12 [2] are introduced via this clause.

Table 3A.2-1: Intra-band contiguous CA configurations

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Feature | DL/UL | CA BW Class | Duplex-mode | Release  independent from | requirements to be fulfilled  (see 36.307 of the REL in which the CA configuration was introduced) |
| Intra-band contiguous CA configurations, power class 3 | DL | B | FDD | Rel-10 | Table B.2.2-1, Table B.3.2-1, Table B.4.2-1 |
| C | FDD, TDD | Rel-10 | Table B.2.2-1, Table B.3.2-1, Table B.4.2-1 |
| D | TDD | Rel-10 | Table B.2.2-1, Table B.3.2-1, Table B.4.2-1 |
| E | TDD | Rel-11 | Table B.2.2-1, Table B.3.2-1, Table B.4.2-1 |
| F | TDD | Rel-12 | Table B.2.2-1, Table B.3.2-1, Table B.4.2-1 |
| UL | B | FDD | Rel-10 | Table B.2.2-1, Table B.3.2-1, Table B.4.2-1 |
| C, D | FDD, TDD | Rel-10 | Table B.2.2-1, Table B.3.2-1, Table B.4.2-1 |
| Intra-band contiguous CA configurations, power class 2 | UL | C | TDD | Rel-10 | Table B.2.2-1, Table B.3.2-1, Table B.4.2-1 |
| NOTE1: The duplex mode "FDD, TDD" refers to a CA configuration composed by only FDD bands or only TDD bands, respectively. | | | | | |

Table 3A.2-2: Inter-band CA configurations

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| Feature | DL/UL | number of bands | number of CCs | CA BW Classes | Duplex-mode | Release  independent from | requirements to be fulfilled  (see 36.307 of the REL in which the CA configuration was introduced) |
| Inter-band CA configurations | DL | 2 | 2-4 | A, B, C | FDD, TDD | Rel-10 | Table B.2.4-1, Table B.3.2-1, Table B.4.3-1 or Table B.4.4-1 |
| 2-5 | D, E | FDD, TDD | Rel-11 | Table B.2.4-1, Table B.3.2-1, Table B.4.3-1 or Table B.4.4-1 |
| 2-5 | A, B, C, D, E | FDD and TDD | Rel-12 | Table B.2.4-1, Table B.3.2-1, Table B.4.3-1 or Table B.4.4-1 |
| 3 | 3 | A | FDD, TDD | Rel-10 | Table B.2.4-1, Table B.3.2-1, Table B.4.3-1 or Table B.4.4-1 |
| 3-5 | B, C, D | FDD, TDD | Rel-11 | Table B.2.4-1, Table B.3.2-1, Table B.4.3-1 or Table B.4.4-1 |
| 3 | A | FDD and TDD | Rel-12 | Table B.2.4-1, Table B.3.2-1, Table B.4.3-1 or Table B.4.4-1 |
| 4 | 4-5 | A, C | FDD, TDD | Rel-11 | Table B.2.4-1, Table B.3.2-1, Table B.4.3-1 or Table B.4.4-1 |
| 4-5 | FDD and TDD | Rel-12 | Table B.2.4-1, Table B.3.2-1, Table B.4.3-1 or Table B.4.4-1 |
| 5 | 5 | A | FDD, TDD | Rel-12 | Table B.2.4-1, Table B.3.2-1, Table B.4.3-1 or Table B.4.4-1 |
| 5 | FDD and TDD | Rel-12 | Table B.2.4-1, Table B.3.2-1, Table B.4.3-1 or Table B.4.4-1 |
| UL | 2 | 2-4 | A, C | FDD, TDD | Rel-11 | Table B.2.4-1, Table B.3.2-1, Table B.4.3-1 or Table B.4.4-1 |
| 2-3 | A, C | FDD and TDD | Rel-12 | Table B.2.4-1, Table B.3.2-1, Table B.4.3-1 or Table B.4.4-1 |
| NOTE1: The duplex mode "FDD, TDD" refers to a CA configuration composed by only FDD bands or only TDD bands, respectively. The duplex mode "FDD and TDD" refers to a CA configuration including both FDD and TDD bands. | | | | | | | |

For example, CA configuration CA\_1A-19A was introduced in the Release 11 specifications. In order to implement a UE conforming to Release 10 but supporting the CA configuration CA\_1A-19A, it is necessary for the UE to additionally conform to some parts of the Release 11 specifications (see corresponding Annexes of TS 36.307 Rel-11 which will point to the requirements in the Rel-11 of TS 36.101 [2] or TS 36.133 [3] to be fulfilled), such as the radio frequency and radio resource management requirements for the CA configuration CA\_1A-19A.

Table 3A.2-3: Intra-band non-contiguous CA configurations

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| Feature | DL/UL | number of sub-blocks | number of CCs | CA BW Classes | Duplex-mode | Release  independent from | requirements to be fulfilled  (see 36.307 of the REL in which the CA configuration was introduced) |
| Intra-band non-contiguous CA configurations | DL | 2 | 2-5 | A, C, D | FDD, TDD | Rel-11 | Table B.2.3-1, Table B.3.2-1, Table B.4.5-1 |
| 3 | 3-5 | A, C | FDD, TDD | Rel-11 | Table B.2.3-1, Table B.3.2-1, Table B.4.5-1 |
| UL | 2 | 2 | A | FDD | Rel-11 | Table B.2.3-1, Table B.3.2-1, Table B.4.5-1 |
| NOTE1: The duplex mode "FDD, TDD" refers to a CA configuration composed by only FDD bands or only TDD bands, respectively. | | | | | | | |

## 3A.3 Additional operating bands and/or CA configurations for specific features

For a specific feature introduced in an earlier release, it may be decided in a later release to apply this specific feature in a release independent way for additional operating bands and/or CA configurations. For a Rel-12 UE corresponding requirements are then introduced via this clause.

Table 3A.3-1: Operating bands for specific features

|  |  |  |  |
| --- | --- | --- | --- |
| Feature | Release  independent from | Requirements to be fulfilled  (see 36.307 of the REL when the feature was introduced) | Further information |
| Operating bands for UE category 0 | Rel-12 | Table B.2.9-1, Table B.3.5-1, Table B.4.10-1 | Rel-14 WI LC\_MTC\_LTE\_cat0\_B25\_B26-Core introduced RF, RRM, demodulation and CSI requirements for bands 25 and 26, see Table B.2.9-1, Table B.3.5-1, Table B.4.10-1 |

Table 3A.3-2: CA configurations for specific features

|  |  |  |  |
| --- | --- | --- | --- |
| Feature | Release  independent from | Requirements to be fulfilled  (see 36.307 of the REL when the feature was introduced) | Further information |
|  |  |  |  |

## 3A.4 Other release independent features

This clause covers requirements for a Rel-12 UE coming from all other release independent features that are not covered under clause 3A.1, 3A.2 and 3A.3, e.g. generic baseband requirements or requirements that are not band/CA configuration specific.

Table 3A.4-1: Additional requirements of other release independent features

|  |  |  |  |
| --- | --- | --- | --- |
| Feature | Release  independent from | Requirements to be fulfilled  (see 36.307 of the REL when the feature was introduced) | Further information |
| RF and performance requirements for 4Rx UEs | Rel-10 | Table C.1-1, Table C.2-1 for single carrier and Table C.1-2, Table C.2-2 for CA | REL-13 WI LTE\_4Rx\_AP\_DL introduced:  - single carrier RF requirements for bands 1, 2, 3, 7, 20, 39, 41, 42: see Table C.1-1  - CA RF requirements for CA\_3A-42A and other 1UL CA configurations (see TS 36.101 REL-13 [2] Table 7.3.1A-0a NOTE 20): see Table C.1-2  - single carrier performance requirements for demodulation and CSI: see Table C.2-1  REL-14 WI LTE\_4Rx\_AP\_DL\_bands introduced:  - single carrier RF requirements for band 35, 40: see Table C.1-1  - CA RF requirements for some further 1UL CA configurations (see TS 36.101 REL-14 [2]): see Table C.1-2  REL-14 WI LTE\_4Rx\_AP\_DL\_CA introduced:  - CA RF requirements for some 2DL/2UL CA configurations (see TS 36.101 REL-14 [2]): see Table C.1-2  - CA performance requirements for demodulation/SDR and CSI: see Table C2-2  REL-15 WI LTE\_4Rx\_AP\_DL\_bands\_R15 introduced:  - single carrier RF requirements for band 4, 34, 43, 66: see Table C.1-1  - CA RF requirements for some further 1UL CA configurations (see TS 36.101 REL-15 [2]): see Table C.1-2 |

# 4 - 292 Void

Annex A (informative) :  
Frequency arrangement for overlapping operating bands

The following information is provided in order to assist a UE derive the DL EARFCN and UL EARFCN in a multi-band environment, in which multiple overlapping operating bands may be indicated in the fields *freqBandIndicator* and *multiBandInfoList* of SIB1.

The overlapping bands, independent of release, which may be indicated in a cell are shown in Table A-1 for applicable E-UTRA bands. The DL EARFCN and UL EARFCN are derived according to TS 36.101 Rel-12 [2].

Table A-1: Overlapping bands (multi-band environments) for each E-UTRA band

|  |  |  |
| --- | --- | --- |
| E-UTRA Operating Band | Overlapping E-UTRA operating bands | Duplex Mode |
| 2 | 25 | FDD |
| 3 | 9 | FDD |
| 4 | 10 | FDD |
| 5 | 18, 19, 26 | FDD |
| 9 | 3 | FDD |
| 10 | 4 | FDD |
| 12 | 17 | FDD |
| 17 | 12 | FDD |
| 18 | 5, 26, 27 | FDD |
| 19 | 5, 26 | FDD |
| 25 | 2 | FDD |
| 26 | 5, 18, 19, 27 | FDD |
| 27 | 18, 26 | FDD |
| 33 | 39 | TDD |
| 38 | 41 | TDD |
| 39 | 33 | TDD |
| 41 | 38 | TDD |

Annex B (normative):  
Common Requirements

# B.1 Purpose of annex

The purpose of Annex B is to group the requirements that are common for several bands or CA configurations in this specification and use the common tables as references.

# B.2 Common RRM requirements

## B.2.1 Common RRM requirements for a release independent band

The requirements and test cases listed in Table B.2.1-1 are specified in TS 36.133 Rel-12 [3].

Table B.2.1-1: Common RRM requirements for a release independent band

|  |  |
| --- | --- |
| Section / Clause | Description |
| 4 Note 1 | E-UTRAN RRC\_IDLE state mobility |
| 5 | E-UTRAN RRC\_CONNECTED state mobility |
| 6 Note 2 | RRC Connection Mobility Control |
| 7 Note 3 | Timing and signalling characteristics |
| 8 Note 4 | UE Measurements Procedures in RRC\_CONNECTED State |
| 9 Note 5 | Measurements performance requirements for UE |
| A.4 Note 1 | E-UTRAN RRC\_IDLE state |
| A.5 | E-UTRAN RRC CONNECTED Mode Mobility |
| A.6 Note 2 | RRC Connection Control |
| A.7 Note 3 | Timing and Signalling Characteristics |
| A.8 Note 4 | UE Measurements Procedures |
| A.9 Note 5 | Measurement Performance Requirements |
| NOTE 1: All requirements and the corresponding test cases shall apply, except:  - for supporting the corresponding band in Rel-9 and below: clause 4.3 (Minimization of Drive Tests).  NOTE 2: All requirements and the corresponding test cases shall apply, except:  - for supporting the corresponding band in Rel-8: clauses 6.3 (RRC Connection Release with Redirection), 6.4 (CSG Proximity Indication for E-UTRAN and UTRAN).  NOTE 3: All requirements and corresponding test cases shall apply, except those defined in sections 7.4 and 7.5.  NOTE 4: All requirements and corresponding test cases shall apply, except:  - for supporting the corresponding band in Rel-8: clauses 8.1.2.5 (E-UTRAN OTDOA Intra-Frequency RSTD Measurements), 8.1.2.6 (E-UTRAN Inter-Frequency OTDOA Measurements), 8.1.2.7 (E-UTRAN E-CID Measurements).  NOTE 5: All requirements and corresponding test cases shall apply, except:  - for supporting the corresponding band in Rel-8: clauses 9.1.9 (UE Rx–Tx time difference), 9.1.10 (Reference Signal Time Difference).  - for supporting the corresponding band in Rel-11 or below: the RSRP absolute accuracy requirement under normal conditions in table 9.1.2.1-1, 9.1.2.3-1, 9.1.2.5-1 and 9.1.3.1-1 when Io≤-70dBm is ±6dB.  - for supporting the corresponding band in Rel-11 or below: the interfrequency RSRP relative accuracy requirement under normal conditions in table 9.1.3.2-1 is ±6dB.  NOTE 6: In addition to the exceptions above, all requirements and test cases in this table shall apply, except those defined for:  - carrier aggregation;  - for supporting the corresponding band in Rel-9 or below: measurements under time-domain measurement resource restriction without CRS assistance information;  - for supporting the corresponding band in Rel-10 or below: measurements under time-domain measurement resource restriction with CRS assistance information;  - for supporting the corresponding band in Rel-11 or below: requirements introduced in Rel-12. | |

## B.2.2 Common RRM requirements for an intra-band contiguous CA configuration

The requirements and test cases listed in Table B.2.2-1 are specified in TS 36.133 Rel-12 [3].

Table B.2.2-1: Common RRM requirements for a release independent single-band CA configuration

|  |  |
| --- | --- |
| Section / Clause | Description |
| 7.1 | UE transmit timing |
| 7.7 | SCell Activation and Deactivation Delay for E-UTRA Carrier Aggregation |
| 7.8 | Interruptions with Carrier Aggregation |
| 8.2 | Capabilities for Support of Event Triggering and Reporting Criteria |
| 8.3 | Measurements for E-UTRA carrier aggregation |
| 8.4 | OTDOA RSTD Measurements for E-UTRAN carrier aggregation |
| 9.1.11 Note 3 | Carrier aggregation measurement accuracy |
| 9.1.12 | Reference Signal Time Difference (RSTD) Measurement Accuracy Requirements for Carrier Aggregation |
| A.7 | Timing and Signalling Characteristics |
| A.8 | UE Measurements Procedures |
| A.9 Note 3 | Measurement Performance Requirements |
| NOTE 1: Only requirements and test cases defined for intra-band contiguous carrier aggregation shall apply.  NOTE 2: In addition to the exceptions above, all requirements and test cases in this table shall apply, except:  - for supporting the corresponding band in Rel-11 or below: requirements introduced in Rel-12.  NOTE 3: - For supporting the corresponding band in Rel-11 or below: the RSRP absolute accuracy requirement under normal conditions in table 9.1.2.1-1, 9.1.2.3-1, 9.1.2.5-1 and 9.1.3.1-1 when Io≤-70dBm is ±6dB.  - For supporting the corresponding band in Rel-11 or below: the interfrequency RSRP relative accuracy requirement under normal conditions in table 9.1.3.2-1 is ±6dB. | |

## B.2.3 Common RRM requirements for an intra-band non-contiguous CA with single uplink configuration

The requirements and test cases listed in Table B.2.3-1 are specified in TS 36.133 Rel-12 [3].

Table B.2.3-1: Common RRM requirements for a release independent single-band CA configuration

|  |  |
| --- | --- |
| Section / Clause | Description |
| 7.1 | UE transmit timing |
| 7.7 | SCell Activation and Deactivation Delay for E-UTRA Carrier Aggregation |
| 7.8 | Interruptions with Carrier Aggregation |
| 8.2 | Capabilities for Support of Event Triggering and Reporting Criteria |
| 8.3 | Measurements for E-UTRA carrier aggregation |
| 8.4 | OTDOA RSTD Measurements for E-UTRAN carrier aggregation |
| 9.1.11 Note 3 | Carrier aggregation measurement accuracy |
| 9.1.12 | Reference Signal Time Difference (RSTD) Measurement Accuracy Requirements for Carrier Aggregation |
| A.7 | Timing and Signalling Characteristics |
| A.8 | UE Measurements Procedures |
| A.9 Note 3 | Measurement Performance Requirements |
| NOTE 1: Only requirements and test cases defined for intra-band non-contiguous carrier aggregation with single uplink shall apply.  NOTE 2: In addition to the exceptions above, all requirements and test cases in this table shall apply, except:  - for supporting the corresponding band in Rel-11 or below: requirements introduced in Rel-12.  NOTE 3: - For supporting the corresponding band in Rel-11 or below: the RSRP absolute accuracy requirement under normal conditions in table 9.1.2.1-1, 9.1.2.3-1, 9.1.2.5-1 and 9.1.3.1-1 when Io≤-70dBm is ±6dB  - for supporting the corresponding band in Rel-11 or below: the interfrequency RSRP relative accuracy requirement under normal conditions in table 9.1.3.2-1 is ±6dB. | |

## B.2.4 Common RRM requirements for an inter-band CA with single uplink configuration

The requirements and test cases listed in Table B.2.4-1 are specified in TS 36.133 Rel-12 [3].

Table B.2.4-1: Common RRM requirements for a release independent band-combination CA configuration

|  |  |
| --- | --- |
| Section / Clause | Description |
| 7.1 | UE transmit timing |
| 7.7 | SCell Activation and Deactivation Delay for E-UTRA Carrier Aggregation |
| 7.8 | Interruptions with Carrier Aggregation |
| 8.2 | Capabilities for Support of Event Triggering and Reporting Criteria |
| 8.3 | Measurements for E-UTRA carrier aggregation |
| 8.4 | OTDOA RSTD Measurements for E-UTRAN carrier aggregation |
| 9.1.11 Note 3 | Carrier aggregation measurement accuracy |
| 9.1.12 | Reference Signal Time Difference (RSTD) Measurement Accuracy Requirements for Carrier Aggregation |
| A.7 | Timing and Signalling Characteristics |
| A.8 | UE Measurements Procedures |
| A.9 Note 3 | Measurement Performance Requirements |
| NOTE 1: Only requirements and test cases defined for inter-band with single uplink carrier aggregation shall apply.  NOTE 2: In addition to the exceptions above, all requirements and test cases in this table shall apply, except:  - for supporting the corresponding band in Rel-11 or below: requirements introduced in Rel-12.  NOTE 3: - For supporting the corresponding band in Rel-11 or below: the RSRP absolute accuracy requirement under normal conditions in table 9.1.2.1-1, 9.1.2.3-1, 9.1.2.5-1 and 9.1.3.1-1 when Io≤-70dBm is ±6dB.  - for supporting the corresponding band in Rel-11 or below: the interfrequency RSRP relative accuracy requirement under normal conditions in table 9.1.3.2-1 is ±6dB. | |

## B.2.5 Common RRM requirements for an inter-band CA with dual uplink configuration

The requirements and test cases listed in Table B.2.5-1 are specified in TS 36.133 Rel-12 [3].

Table B.2.5-1: Common RRM requirements for a release independent band-combination CA configuration with dual uplink

|  |  |
| --- | --- |
| Section / Clause | Description |
| 7.1 | UE transmit timing |
| 7.7 | SCell Activation and Deactivation Delay for E-UTRA Carrier Aggregation |
| 7.8 | Interruptions with Carrier Aggregation |
| 7.17 | Maximum Transmission Timing Difference in Dual Connectivity |
| 8.2 | Capabilities for Support of Event Triggering and Reporting Criteria |
| 8.3 | Measurements for E-UTRA carrier aggregation |
| 8.4 | OTDOA RSTD Measurements for E-UTRAN carrier aggregation |
| 9.1.11 Note 3 | Carrier aggregation measurement accuracy |
| 9.1.12 | Reference Signal Time Difference (RSTD) Measurement Accuracy Requirements for Carrier Aggregation |
| A.7 | Timing and Signalling Characteristics |
| A.8 | UE Measurements Procedures |
| A.9 Note 3 | Measurement Performance Requirements |
| NOTE 1: Only requirements and test cases defined for inter-band with dual uplink carrier aggregation shall apply.  NOTE 2: In addition to the exceptions above, all requirements and test cases in this table shall apply, except:  - for supporting the corresponding band in Rel-11 or below: requirements introduced in Rel-12.  NOTE 3: - For supporting the corresponding band in Rel-11 or below: the RSRP absolute accuracy requirement under normal conditions in table 9.1.2.1-1, 9.1.2.3-1, 9.1.2.5-1 and 9.1.3.1-1 when Io≤-70dBm is ±6dB.  - for supporting the corresponding band in Rel-11 or below: the interfrequency RSRP relative accuracy requirement under normal conditions in table 9.1.3.2-1 is ±6dB. | |

## B.2.6 Common RRM requirements for an intra-band non-contiguous CA with dual uplink configuration

The requirements and test cases listed in Table B.2.6-1 are specified in TS 36.133 Rel-12 [3].

Table B.2.6-1: Common RRM requirements for a release independent single-band CA configuration with dual uplink

|  |  |
| --- | --- |
| Section / Clause | Description |
| 7.1 | UE transmit timing |
| 7.7 | SCell Activation and Deactivation Delay for E-UTRA Carrier Aggregation |
| 7.17 | Maximum Transmission Timing Difference in Dual Connectivity |
| 7.8 | Interruptions with Carrier Aggregation |
| 8.2 | Capabilities for Support of Event Triggering and Reporting Criteria |
| 8.3 | Measurements for E-UTRA carrier aggregation |
| 8.4 | OTDOA RSTD Measurements for E-UTRAN carrier aggregation |
| 9.1.11 Note 3 | Carrier aggregation measurement accuracy |
| 9.1.12 | Reference Signal Time Difference (RSTD) Measurement Accuracy Requirements for Carrier Aggregation |
| A.7 | Timing and Signalling Characteristics |
| A.8 | UE Measurements Procedures |
| A.9 Note 3 | Measurement Performance Requirements |
| NOTE 1: Only requirements and test cases defined for intra-band non-contiguous carrier aggregation with dual uplinks shall apply.  NOTE 2: In addition to the exceptions above, all requirements and test cases in this table shall apply, except:  - for supporting the corresponding band in Rel-11 or below: requirements introduced in Rel-12.  NOTE 3: - For supporting the corresponding band in Rel-11 or below: the RSRP absolute accuracy requirement under normal conditions in table 9.1.2.1-1, 9.1.2.3-1, 9.1.2.5-1 and 9.1.3.1-1 when Io≤-70dBm is ±6dB.  - for supporting the corresponding band in Rel-11 or below: the interfrequency RSRP relative accuracy requirement under normal conditions in table 9.1.3.2-1 is ±6dB. | |

## B.2.7 Void

## B.2.8 Void

## B.2.9 Void

# B.3 Common UE performance requirements

## B.3.1 Void

## B.3.2 Common UE performance requirements and tests for different CA configurations and combination sets

The requirements and test cases listed in Table B.3.2-1 are specified in TS 36.101 Rel-12 [2].

Table B.3.2-1: Common UE performance requirements and tests for release independent CA configurations and combination sets

|  |  |
| --- | --- |
| Section / Clause | Description |
| 8.2.1.1.1 | Single-antenna port performance (FDD) |
| 8.2.2.1.1 | Single-antenna port performance (TDD) |
| 8.2.1.3.1 | Open-loop spatial multiplexing performance - Minimum Requirement 2 Tx Antenna Port (FDD) |
| 8.2.2.3.1 | Open-loop spatial multiplexing performance - Minimum Requirement 2 Tx Antenna Port (TDD) |
| 8.2.1.3.1A | Open-loop spatial multiplexing performance - Soft buffer management test (FDD) |
| 8.2.2.3.1A | Open-loop spatial multiplexing performance - Soft buffer management test (TDD) |
| 8.2.1.4.3 | Closed-loop spatial multiplexing performance - Minimum Requirement Multi-Layer Spatial Multiplexing 4 Tx Antenna Port (FDD) |
| 8.2.1.4.3A | Closed-loop spatial multiplexing performance - Minimum Requirement Multi-Layer Spatial Multiplexing 4 Tx Antenna Port (DC) |
| 8.2.2.4.3 | Closed-loop spatial multiplexing performance - Minimum Requirement Multi-Layer Spatial Multiplexing 4 Tx Antenna Port (TDD) |
| 8.2.2.4.4 | Closed-loop spatial multiplexing performance - Minimum Requirement Multi-Layer Spatial Multiplexing 4 Tx Antenna Port (DC) |
| 8.2.1.7 | Carrier aggregation with power imbalance (FDD) |
| 8.2.1.8 | Intra-band non-contiguous carrier aggregation with timing offset (FDD) |
| 8.2.2.7 | Carrier aggregation with power imbalance (TDD) |
| 8.7.1 | Sustained downlink data rate provided by lower layers (FDD) |
| 8.7.2 | Sustained downlink data rate provided by lower layers (TDD) |
| 8.7.5 | Sustained downlink data rate provided by lower layers (TDD-FDD CA) |
| 9.6.1.1 | Additional requirements for carrier aggregation - Periodic reporting on multiple cells (Cell Specific Reference symbols) (FDD) |
| 9.6.1.2 | Additional requirements for carrier aggregation - Periodic reporting on multiple cells (Cell Specific Reference symbols) (TDD) |
| NOTE 1: The applicability of requirements for different CA configurations and bandwidth combination sets is specified in Section 8.1.2.3 and 9.1.1.2.  NOTE 2: The test coverage for different number of component carriers is defined in 8.1.2.4. | |

## B.3.3 Void

## B.3.4 Void

## B.3.5 Void

# B.4 Common UE RF requirements

## B.4.1 Common UE RF requirements for a release independent band

The requirements and test cases listed in Table B.4.1-1 are specified in TS 36.101 Rel-12 [2].

Table B.4.1-1: Common UE RF requirements for a release independent band

|  |  |
| --- | --- |
| Section / Clause | Description |
| 5.5 | Operating bands |
| 5.6 | Channel bandwidth |
| 5.7 | Channel arrangement |
| 6.2 | Transmit power |
| 6.3 | Output power dynamics |
| 6.5 | Transmit signal quality |
| 6.6 | Output RF spectrum emissions |
| 6.7 | Transmit intermodulation |
| 7.3 | Reference sensitivity power level |
| 7.4 | Maximum input level |
| 7.5 | Adjacent Channel Selectivity (ACS) |
| 7.6 | Blocking characteristics |
| 7.7 | Spurious response |
| 7.8 | Intermodulation characteristics |
| 7.9 | RX spurious emissions |

## B.4.2 Common UE RF requirements for an intra-band contiguous CA configuration

The requirements and test cases listed in Table B.4.2-1 are specified in TS 36.101 Rel-12 [2].

Table B.4.2-1: Common UE RF requirements for a release independent intra-band contiguous CA configuration

|  |  |
| --- | --- |
| Section / Clause | Description |
| 5.5A | Operating bands for CA |
| 5.6A | Channel bandwidths per operating band for CA |
| 5.7.1A | Channel spacing for CA |
| 5.7.2A | Channel raster for CA |
| 5.7.4A | TX–RX frequency separation for CA |
| 6.2.2A | UE maximum output power for CA |
| 6.2.3A | UE maximum output power for modulation/channel bandwidth for CA |
| 6.2.4A | UE maximum output power with additional requirements for CA |
| 6.2.5A | Configured transmitted power for CA |
| 6.3.2A | UE Minimum utput power for CA |
| 6.3.3A | UE Trasnsmit OFF power for CA |
| 6.3.4A | ON/OFF time mask for CA |
| 6.3.5A | Power control for CA |
| 6.5.1A | Frequency error for CA |
| 6.5.2A | Transmit modulation quality for CA |
| 6.6.1A | Occupied bandwidth for CA |
| 6.6.2.1A | Spectrum emission mask for CA |
| 6.6.2.2A | Additional Spectrum Emission mask for CA |
| 6.6.2.3.2A | UTRA ACLR for CA |
| 6.6.2.3.3A | E-UTRA ACLR for CA |
| 6.6.3.1A | Minimum requirements for CA |
| 6.6.3.2A | Spurious emission band UE co-existence for CA |
| 6.6.3.3A | Additional spurious emissions for CA |
| 6.7.1A | Minimum requirement for CA |
| 7.3.1A | Reference sensitivity for CA |
| 7.4.1A | Maximum input level for CA |
| 7.5.1A | Adjacent Channel Selectivity (ACS) for CA |
| 7.6.1.1A | In-band blocking for CA |
| 7.6.2.1A | Out-of-band blocking for CA |
| 7.6.3.1A | Narrow band blocking for CA |
| 7.7.1A | Spurious response for CA |
| 7.8.1A | Wideband intermodulation for CA |
| 7.10.1A | Receiver response for CA |

## B.4.3 Common UE RF requirements for an single uplink inter-band CA configuration

The requirements and test cases listed in Table B.4.3-1 are specified in TS 36.101 Rel-12 [2].

Table B.4.3-1: Common UE RF requirements for a release independent inter-band CA configuration

|  |  |
| --- | --- |
| Section / Clause | Description |
| 5.5A | Operating bands for CA |
| 5.6A.1 | Channel bandwidths per operating band for CA |
| 5.7.2A | Channel raster for CA |
| 6.2.2A | UE maximum output power for CA |
| 6.2.3A | UE maximum output power for modulation/channel bandwidth for CA |
| 6.2.5 | Configured transmitted power |
| 7.3.1A | Reference sensitivity for CA |
| 7.4.1A | Maximum input level for CA |
| 7.5.1A | Adjacent Channel Selectivity (ACS) for CA |
| 7.6.1.1A | In-band blocking for CA |
| 7.6.2.1A | Out-of-band blocking for CA |
| 7.6.3.1A | Narrow band blocking for CA |
| 7.7.1A | Spurious response for CA |
| 7.8.1A | Wideband intermodulation for CA |

## B.4.4 Common UE RF requirements for an inter-band CA configuration including an operating band without uplink band

The requirements and test cases listed in Table B.4.4-1 are specified in TS 36.101 Rel-12 [2].

Table B.4.4-1: Common UE RF requirements for a release independent inter-band CA configuration including an operating band without uplink band

|  |  |
| --- | --- |
| Section / Clause | Description |
| 5.5 | Operating bands |
| 5.5A | Operating bands for CA |
| 5.6A.1 | Channel bandwidths per operating band for CA |
| 5.7 | Channel arrangement |
| 6.2.2A | UE maximum output power for CA |
| 6.2.3A | UE maximum output power for modulation/channel bandwidth for CA |
| 6.2.5 | Configured transmitted power |
| 7.3.1A | Reference sensitivity for CA |
| 7.4.1A | Maximum input level for CA |
| 7.5.1A | Adjacent Channel Selectivity (ACS) for CA |
| 7.6.1.1A | In-band blocking for CA |
| 7.6.2.1A | Out-of-band blocking for CA |
| 7.6.3.1A | Narrow band blocking for CA |
| 7.7.1A | Spurious response for CA |
| 7.8.1A | Wideband intermodulation for CA |

## B.4.5 Common UE RF requirements for a single uplink intra-band non-contiguous CA configuration

The requirements and test cases listed in Table B.4.5-1 are specified in TS 36.101 Rel-12 [2].

Table B.4.5-1: Common UE RF requirements for a release independent single uplink intra-band non-contiguous CA configuration

|  |  |
| --- | --- |
| Section / Clause | Description |
| 5.5A | Operating bands for CA |
| 5.6A1 | Channel bandwidths per operating band for CA |
| 5.7.2A | Channel raster for CA |
| 6.2.2A | UE maximum output power for CA |
| 6.2.3A | UE maximum output power for modulation/channel bandwidth for CA |
| 7.3.1A | Reference sensitivity for CA |
| 7.4.1A | Maximum input level for CA |
| 7.5.1A | Adjacent Channel Selectivity (ACS) for CA |
| 7.6.1.1A | In-band blocking for CA |
| 7.6.2.1A | Out-of-band blocking for CA |
| 7.6.3.1A | Narrow band blocking for CA |
| 7.7.1A | Spurious response for CA |
| 7.8.1A | Wideband intermodulation for CA |

## B.4.6 Common UE RF requirements for a dual uplink inter-band CA configuration

The requirements and test cases listed in Table B.4.6-1 are specified in TS 36.101 Rel-12 [2].

Table B.4.6-1: Common UE RF requirements for a release independent dual uplink inter-band CA configuration

|  |  |
| --- | --- |
| Section / Clause | Description |
| 5.6A.1 | Channel bandwidths per operating band for CA |
| 6.2.2A | UE maximum output power for CA |
| 6.2.5A | Configured transmitted Power for CA |
| 6.3.2A | UE Minimum output power for CA |
| 6.3.3A | UE Transmit OFF power for CA |
| 6.3.4A | ON/OFF time mask for CA |
| 6.3.5A | Power control for CA |
| 6.5.1A | Frequency error for CA |
| 6.5.2A | Transmit modulation quality for CA |
| 6.6.1A | Occupied bandwidth for CA |
| 6.6.2.1A | Spectrum emission mask for CA |
| 6.6.2.3 | Adjacent Channel Leakage Ratio |
| 6.6.3.1A | Spurious Emission for CA |
| 6.6.3.2A | Spurious emission band UE co-existence for CA |
| 6.7.1A | Transmit intermodulation for CA |
| 7.3.1A | Reference sensitivity for CA |
| 7.6.2.1A | Out-of-band blocking for CA |
| 7.7.1A | Spurious response for CA |

## B.4.7 Common UE RF requirements for a dual uplink intra-band non-contiguous CA configuration

The requirements and test cases listed in Table B.4.7-1 are specified in TS 36.101 Rel-12 [2].

Table B.4.7-1: Common UE RF requirements for a release independent dual uplink intra-band non-contiguous CA configuration

|  |  |
| --- | --- |
| Section / Clause | Description |
| 5.6A.1 | Channel bandwidths per operating band for CA |
| 6.2.2A | UE maximum output power for CA |
| 6.2.3A | UE Maximum Output power for modulation / channel bandwidth for CA |
| 6.2.5A | Configured transmitted Power for CA |
| 6.3.2A | UE Minimum output power for CA |
| 6.3.3A | UE Transmit OFF power for CA |
| 6.3.4A | ON/OFF time mask for CA |
| 6.3.5A | Power control for CA |
| 6.5.1A | Frequency error for CA |
| 6.5.2A | Transmit modulation quality for CA |
| 6.6.1A | Occupied bandwidth for CA |
| 6.6.2.1A | Spectrum emission mask for CA |
| 6.6.2.3 | Adjacent Channel Leakage Ratio |
| 6.6.3.1A | Spurious Emission for CA |
| 6.6.3.2A | Spurious emission band UE co-existence for CA |
| 7.3.1A | Reference sensitivity for CA |
| 7.6.2.1A | Out-of-band blocking for CA |
| 7.7.1A | Spurious response for CA |

## B.4.8 Void

## B.4.9 Void

## B.4.10 Void

Annex C (informative):  
Change history

Table C.1: Change History

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Date** | **Meeting** | **TDoc** | **CR** | **Rev** | **Cat** | **Subject/Comment** | **New version** |
| 11-2009 | RP#46 | RP-091141 |  |  |  | TS36.307 V0.1.0 approved by RAN (Originally in R4-095022) | 0.1.0 |
| 02-2010 | R4#54 | R4-100419 |  |  |  | For release 9 version, replace sections 4 to 6 as ‘Void’ and add a new void section as section 7. | 0.2.0 |
| 03-2010 | RP#47 | RP-100162 |  |  |  | TS36.307 v1.0.0 for approval | 1.0.0 |
| 03-2010 | RP#47 | RP-100162 |  |  |  | Approved by RAN | 9.0.0 |
| 09-2010 | RP-49 | RP-100927 | 2 |  |  | CR LTE\_TDD\_2600\_US spectrum band definition additions to TS 36.307 V900 | 9.1.0 |
|  |  |  |  |  |  | Correction of section numbering | 9.1.1 |
| 12-2010 | RP-50 | RP-101356 | 008 |  |  | Band 42 and 43 parameters for UMTS/LTE 3500 (TDD) for TS 36.307 | 9.2.0 |
| 12-2010 | RP-50 | RP-101361 | 005 |  |  | Introduction of L-band in TS 36.307 | 9.2.0 |
| 12-2010 | RP-50 | RP-101344 | 016 |  |  | CR creating the rel-10 of the 36.307 specification | 9.3.0 |
| 12-2010 | RP-50 | RP-101356 | 012 |  |  | Band 42 and 43 parameters for UMTS/LTE 3500 (TDD) for TS 36.307 | 9.3.0 |
| 12-2010 | RP-50 |  |  |  |  | Raised to Rel-10 with no technical change | 10.0.0 |
| 01-2011 |  |  |  |  |  | Correction to history table | 10.0.1 |
| 06-2011 | RP-52 | RP-110804 | 015 |  |  | Add Expanded 1900 MHz Band (Band 25) in 36.307 | 10.1.0 |
| 06-2011 | RP-52 | RP-110812 | 022 |  |  | Add 2GHz S-Band (Band 23) in 36.307 (Rel 10) | 10.1.0 |
| 09-2011 | RP-53 | RP-111255 | 025 |  |  | Add Band 22 for LTE/UMTS 3500 (FDD) to TS 36.307 | 10.2.0 |
| 03-2012 | RP-55 | RP-120305 | 029 |  |  | Introduction of Band 26/XXVI to TS 36.307 | 11.0.0 |
| 2012-06 | RP-56 | RP-120789 | 043 |  |  | Introduction of CA\_1A-19A to TS 36.307 | 11.1.0 |
| 2012-06 | RP-56 | RP-120793 | 049 |  |  | Introduction of APAC700(FDD) into TS 36.307 Rel-11 | 11.1.0 |
| 2012-06 | RP-56 | RP-120793 | 053 |  |  | Introduction of APAC700(TDD) into TS 36.307 Rel-11 | 11.1.0 |
| 2012-06 | RP-56 | RP-120791 | 057 |  |  | Introduction of e850\_LB (Band 27) to TS 36.307 | 11.1.0 |
| 2012-09 | RP-57 | RP-121335 | 059 |  |  | Introduction of CA\_1A-21A to TS 36.307 | 11.2.0 |
| 2012-09 | RP-57 | RP-121295 | 070r1 |  |  | Relation between EARFCN for overlapping bands with multiple FBI indication | 11.2.0 |
| 2012-09 | RP-57 | RP-121338 | 072 |  |  | 36.307 CR for LTE\_CA\_B7 | 11.2.0 |
| 2012-09 | RP-57 | RP-121337 | 073 |  |  | TS 36.307 CR for CA\_38 | 11.2.0 |
| 2012-09 | RP-57 | RP-121327 | 074 |  |  | Introduction of CA\_B7\_B20 in 36.307 | 11.2.0 |
| 2012-09 | RP-57 | RP-121329 | 075 |  |  | Introduction of CA band combination Band3 + Band5 to TS 36.307 | 11.2.0 |
| 2012-09 | RP-57 | RP-121331 | 076 |  |  | Introduction of CA\_3A-20A to TS 36.307 | 11.2.0 |
| 2012-09 | RP-57 | RP-121334 | 077 |  |  | Add requirements for inter-band CA of B\_1-18 in TS36.307 | 11.2.0 |
| 2012-09 | RP-57 | RP-121333 | 078 |  |  | Introduction of CA\_8\_20 RF requirements into TS36.307 | 11.2.0 |
| 2012-09 | RP-57 | RP-121324 | 079 |  |  | Introduction of CA\_B3\_B7 in 36.307 | 11.2.0 |
| 2012-12 | RP-58 | RP-121890 | 086 |  |  | Introduction of CA\_4A-5A into 36.307 | 11.3.0 |
| 2012-12 | RP-58 | RP-121889 | 088 |  |  | Introduction of CA band combination Band4 + Band13 to TS 36.307 (Rel-11) | 11.3.0 |
| 2012-12 | RP-58 | RP-121896 | 091 |  |  | Introduction of Band 5 + Band 17 inter-band CA configuration into 36.307 | 11.3.0 |
| 2012-12 | RP-58 | RP-121884 | 092 |  |  | Introduction of CA\_3A-8A to TS 36.307 | 11.3.0 |
| 2012-12 | RP-58 | RP-121894 | 093 |  |  | Introduction of CA\_B5\_B12 in 36.307 | 11.3.0 |
| 2012-12 | RP-58 | RP-121887 | 095 |  |  | Introduction of CA\_4-12 into TS 36.307 (Rel-11) | 11.3.0 |
| 2012-12 | RP-58 | RP-121882 | 097 |  |  | [Rel-11] Introduction of inter-band CA\_11-18 into TS36.307 | 11.3.0 |
| 2012-12 | RP-58 | RP-121861 | 099 |  |  | Release-independent implementation of carrier aggregation configuration CA\_4-7 | 11.3.0 |
| 2012-12 | RP-58 | RP-121901 | 101 |  |  | Introduction of Band 29 | 11.3.0 |
| 2012-12 | RP-58 | RP-121718 | 0102 |  |  | Introduction of CA band combination Band2 + Band17 to TS 36.307 (Rel-11) | 11.3.0 |
| 2012-12 | RP-58 | RP-121720 | 0104 |  |  | Introduction of CA band combination Band4 + Band17 to TS 36.307 (Rel-11) | 11.3.0 |
| 2013-06 | RP-60 | RP-130771 | 108 |  |  | Introduction of CA 1+8 into TS36.307(Rel-12) | 12.0.0 |
| 2013-06 | RP-60 | RP-130782 | 111 |  |  | Introduction of LTE Advanced inter-band Carrier Aggregation of Band 3 and Band 28 to TS 36.307 Rel-12 | 12.0.0 |
| 2013-06 | RP-60 | RP-130785 | 114 |  |  | Introduction of LTE Advanced inter-band Carrier Aggregation of Band 23 and Band 29 to TS 36.307 (Rel-12) | 12.0.0 |
| 2013-06 | RP-60 | RP-130779 | 117 |  |  | Introduction of LTE Advanced inter-band Carrier Aggregation of Band 3 and Band 26 to TS 36.307 (Rel-12) | 12.0.0 |
| 2013-06 | RP-60 | RP-130777 | 120 |  |  | Introduction of CA\_3A-19A to TS 36.307 | 12.0.0 |
| 2013-06 | RP-60 | RP-130783 | 123 |  |  | Introduction of CA\_19A-21A to TS 36.307 | 12.0.0 |
| 2013-06 | RP-60 | RP-130775 | 131 |  |  | Introduction of CA\_2A-13A to TS 36.307 | 12.0.0 |
| 2013-06 | RP-60 | RP-130791 | 136 |  |  | Introduction of Band 30 | 12.0.0 |
| 2013-06 | RP-60 | RP-130790 | 143 |  |  | Introduction of LTE 450 into TS 36.307 R12 | 12.0.0 |
| 2013-06 | RP-60 | RP-130787 | 150 |  |  | Introduction of CA\_4A-4A into 36.307 Rel-12 | 12.0.0 |
| 09-2013 | RP-61 | RP-131300 | 153 |  |  | 36.307 CR for LTE\_CA\_C\_B3 (Rel-12) | 12.1.0 |
| 09-2013 | RP-61 | RP-131296 | 160 |  |  | [Rel-12] Add requirements for CA\_1A-26A into TS36.307 | 12.1.0 |
| 09-2013 | RP-61 | RP-131297 | 163 |  |  | Introduction of CA\_2A-4A to TS 36.307 | 12.1.0 |
| 09-2013 | RP-61 | RP-131298 | 167 |  |  | Introduction of inter-band CA Band 2+5 | 12.1.0 |
| 12-2013 | RP-62 | RP-131965 | 173 |  |  | Introduction of CA\_23A-23A to TS 36.307 | 12.2.0 |
| 12-2013 | RP-62 | RP-131946 | 178 |  |  | Introduction of CA band combination Band2 + Band12 to TS 36.307 | 12.2.0 |
| 12-2013 | RP-62 | RP-131954 | 181 |  |  | Introduction of CA band combination Band12 + Band25 to TS 36.307 | 12.2.0 |
| 12-2013 | RP-62 | RP-131959 | 184 |  |  | Introduction of LTE\_CA\_C\_B27 to 36.307 (Rel-12) | 12.2.0 |
| 12-2013 | RP-62 | RP-131957 | 192 |  |  | Introduction of CA\_23B to TS 36.307 | 12.2.0 |
| 12-2013 | RP-62 | RP-131961 | 194 |  |  | Introduction of Intra-band non-contiguous CA in band 3 to TS 36.307 | 12.2.0 |
| 12-2013 | RP-62 | RP-131950 | 200 |  |  | Introduction of CA band combination Band5 + Band25 to TS 36.307 | 12.2.0 |
| 12-2013 | RP-62 | RP-131967 | 201r1 |  |  | Introducing 'General' clause with note referring to note in clause 4.4 in TS36.101, editorial corrections and modifications to Forward and Scope clauses | 12.2.0 |
| 12-2013 | RP-62 | RP-131948 | 204 |  |  | Introduction of CA band combination B5 + B7 to TS 36.307 R12 | 12.2.0 |
| 12-2013 | RP-62 | RP-131952 | 207 |  |  | Introduction of CA band combination B7 + B28 to TS 36.307 | 12.2.0 |
| 12-2013 | RP-62 | RP-131967 | 211 |  |  | Correction to release independent specification | 12.2.0 |
| 12-2013 | RP-62 | RP-131925 | 216 |  |  | UE performance requirements in release independent specification for CA | 12.2.0 |
| 12-2013 | RP-62 | RP-131963 | 219 |  |  | Introduction of CA\_7A-7A to TS 36.307 Rel-12 | 12.2.0 |
| 03-2014 | RP-63 | RP-140371 | 235 |  |  | Release independence of Band 14 HPUE | 12.3.0 |
| 03-2014 | RP-63 | RP-140386 | 227 |  |  | Introduction of CA band combination Band 3 and Band 27 to TS 36.307 | 12.3.0 |
| 03-2014 | RP-63 | RP-140389 | 245r1 |  |  | Correction to release independent specification | 12.3.0 |
| 03-2014 | RP-63 | RP-140388 | 210r1 |  |  | Introduction of CA\_39C to TS 36.307 | 12.3.0 |
| 03-2014 | RP-63 | RP-140387 | 197r1 |  |  | Introduction of CA\_39A-41A to TS 36.307 | 12.3.0 |
| 06-2014 | RP-64 | RP-140911 | 259 |  |  | Introduction of CA band combination Band 1 and Band 5 to TS 36.307 | 12.4.0 |
| 06-2014 | RP-64 | RP-140918 | 300 |  |  | Correction of Common RRM requirements for CA in release independent specification (Rel-12) | 12.4.0 |
| 06-2014 | RP-64 | RP-140926 | 280r1 |  |  | Introduction of Band 20+32 CA | 12.4.0 |
| 06-2014 | RP-64 | RP-140931 | 265 |  |  | Introduction of CA 1+11 to 36.307 (Rel-12) | 12.4.0 |
| 06-2014 | RP-64 | RP-140933 | 275 |  |  | Introduction of CA band combination Band 4 and Band 27 to TS 36.307 | 12.4.0 |
| 06-2014 | RP-64 | RP-140938 | 291 |  |  | Introduction of CA\_2A-2A to TS 36.307 Rel-12 | 12.4.0 |
| 06-2014 | RP-64 | RP-140940 | 319 |  |  | Introduction of LTE\_CA\_NC\_B42 into 36.307 | 12.4.0 |
| 06-2014 | RP-64 | RP-140942 | 253 |  |  | Introduction of CA band combination Band 3 and Band 27 to TS 36.307 | 12.4.0 |
| 06-2014 | RP-64 | RP-140942 | 340 |  |  | Introduction of CA band combination Band 1 and Band 20 to TS 36.307 | 12.4.0 |
| 06-2014 | RP-64 | RP-140943 | 347 |  |  | Introduction of CA band combination CA\_41D into TS 36.307 (Rel-12) | 12.4.0 |
| 09-2014 | RP-65 | RP-141110 | 0388r1 |  |  | [Rel-12] Introduction of inter-band CA\_18-28 into TS36.307 | 12.5.0 |
| 09-2014 | RP-65 | RP-141200 | 0366r1 |  |  | Introduction of CA\_B1\_B3\_B19 into TS 36.307 (Rel-12) | 12.5.0 |
| 09-2014 | RP-65 | RP-141205 | 0363r1 |  |  | Introduction of CA\_B1\_B3 into TS 36.307 (Rel-12) | 12.5.0 |
| 09-2014 | RP-65 | RP-141332 | 0429r1 |  |  | Introduction of CA\_1A-7A into 36.307 (Rel -12) | 12.5.0 |
| 09-2014 | RP-65 | RP-141340 | 0376r1 |  |  | Introduction of CA\_B1\_B5\_B7 into TS 36.307 (Rel-12) | 12.5.0 |
| 09-2014 | RP-65 | RP-141467 | 0432 |  |  | Introduction of 3 DL CA for Band 1+7+20 | 12.5.0 |
| 09-2014 | RP-65 | RP-141527 | 415r1 |  |  | CR for 36.307 on CA UE performance requirement in Rel-12 | 12.5.0 |
| 09-2014 | RP-65 | RP-141551 | 360 |  |  | Introduction of CA 8+11 to 36.307 (Rel-12) | 12.5.0 |
| 09-2014 | RP-65 | RP-141552 | 379 |  |  | Introduction of CA\_41A-42A to TS 36.307 | 12.5.0 |
| 09-2014 | RP-65 | RP-141553 | 381 |  |  | Introduction of a new bandwidth combination set for CA\_25A-25A into 36.307 | 12.5.0 |
| 09-2014 | RP-65 | RP-141554 | 418r1 |  |  | Introduction of requirements for 2DL inter-band carrier aggregation (FDD) and 2DL fallback | 12.5.0 |
| 09-2014 | RP-65 | RP-141554 | 421 |  |  | Introduction of requirements for 3DL inter-band carrier aggregation including Band 30 | 12.5.0 |
| 09-2014 | RP-65 | RP-141555 | 384 |  |  | Introduction of 3 Band Carrier Aggregation of Band 1,Band 3 and Band 5 to TS 36.307(Rel.12) | 12.5.0 |
| 09-2014 | RP-65 | RP-141556 | 357r1 |  |  | Introduction of 3 Band Carrier Aggregation (3DL/1UL) of Band 1, Band 3 and Band 8 to TS 36.307 | 12.5.0 |
| 09-2014 | RP-65 | RP-141558 | 402 |  |  | Introduction of CA band combination Band 1, Band 3 and Band 20 to TS 36.307 | 12.5.0 |
| 09-2014 | RP-65 | RP-141560 | 352 |  |  | Introduction of new CA\_40C bandwidth combination set into 36.307 | 12.5.0 |
| 09-2014 | RP-65 | RP-141561 | 354 |  |  | CR to 36.307 Rel-12: Introduction of CA\_41C-41A and CA\_41A-41C | 12.5.0 |
| 12-2014 | RP-66 | RP-142142 | 440 |  |  | UE RF requirements in the release independent spec | 12.6.0 |
| 12-2014 | RP-66 | RP-142188 | 444 |  |  | Revision of common RRM requirements for release independent specification | 12.6.0 |
| 12-2014 | RP-66 | RP-142182 | 448 |  |  | [Rel-12] Introduction of inter-band CA\_1-28 into TS36.307 | 12.6.0 |
| 12-2014 | RP-66 | RP-142189 | 455 |  |  | CR for TR 36.307: LTE\_CA\_B5\_B13 | 12.6.0 |
| 12-2014 | RP-66 | RP-142190 | 458r2 |  |  | Introduction of additional band combinations for 3DL inter-band CA | 12.6.0 |
| 03-2015 | RP-67 | RP-150387 | 463 |  |  | R4-73AH-0113: Correction of UE RF requirements for dual uplik to TS 36.307 Rel-12 | 12.7.0 |
| 03-2015 | RP-67 | RP-150392 | 468 |  |  | CR for 36.307 on CA UE performance requirement in Rel-12 | 12.7.0 |
| 03-2015 | RP-67 | RP-150387 | 469 |  |  | Further revision of RSRP requirement for 36.307 release 12 | 12.7.0 |
| 06-2015 | RP-68 | RP-151026 | 0471r3 |  |  | Introduction of CA\_42D to TS 36.307(Rel-12) | 12.8.0 |
| 06-2015 | RP-68 | RP-151067 | 0510r1 |  |  | Introduction of CA\_3A-40A to TS 36.307 R12 | 12.8.0 |
| 06-2015 | RP-68 | RP-151069 | 0512r1 |  |  | Introduction of CA\_3A-40C to TS 36.307 R12 | 12.8.0 |
| 06-2015 | RP-68 | RP-150958 | 460r1 |  |  | Introduction of dual uplink CA into 36.307 | 12.8.0 |
| 06-2015 | RP-68 | RP-150958 | 487 |  |  | CR for CA UE performance tests in 36.307 in Rel-12 | 12.8.0 |
| 06-2015 | RP-68 | RP-150968 | 498r2 |  |  | Release independence CR for 2DL inter-band CA Rel-12 | 12.8.0 |
| 06-2015 | RP-68 | RP-150972 | 502r1 |  |  | Release independence CR for 3DL inter-band CA Rel-12 | 12.8.0 |
| 06-2015 | RP-68 | RP-150974 | 505r1 |  |  | Release independence CR for 4DL inter-band CA Rel-12 | 12.8.0 |
| 06-2015 | RP-68 | RP-150975 | 508 |  |  | Introduction of non-contiguous Carrier Aggregation (CA) in Band 42 for 3DL | 12.8.0 |
| 09-2015 | RP-69 | RP-151505 | 516 |  |  | Additional bandwidth combination set for LTE Advanced intra-band non-contiguous Carrier Aggregation in Band 4 | 12.9.0 |
| 09-2015 | RP-69 | RP-151501 | 519r1 |  |  | Introduction of finished 4DL inter-band CAs to TS 36.307 | 12.9.0 |
| 09-2015 | RP-69 | RP-151476 | 522r1 |  |  | Correction of TS 36.307 for release independent | 12.9.0 |
| 09-2015 | RP-69 | RP-151503 | 525 |  |  | [Rel-12] Introduction of dual uplink CA into 36.307 | 12.9.0 |
| 09-2015 | RP-69 | RP-151498 | 533r1 |  |  | Rel-13 2DL combinations | 12.9.0 |
| 09-2015 | RP-69 | RP-151499 | 537 |  |  | Rel-13 3DL combinations | 12.9.0 |
| 09-2015 | RP-69 | RP-151504 | 541 |  |  | Introduction of 3DL/2UL inter-band CA combinations without self-interference issues | 12.9.0 |
| 09-2015 | RP-69 | RP-151202 | 544 |  |  | Introduction of CA\_7A-40A and CA\_7A-40C to TS 36.307 R12 | 12.9.0 |
| 12-2015 | RP-70 | RP-152158 | 0544aR2 |  |  | Release independent requirements for CA\_42E (Rel-12) | 12.10.0 |
| 12-2015 | RP-70 | RP-152160 | 0548a |  |  | Introduction of 4DL NC CA in band42 in 36.307 | 12.10.0 |
| 12-2015 | RP-70 | RP-152133 | 0556 |  |  | [Rel-12] Introduction of dual uplink CA into 36.307 | 12.10.0 |
| 12-2015 | RP-70 | RP-152157 | 0560 |  |  | Introducing B20 + B67 CA into TS 36.307 | 12.10.0 |
| 12-2015 | RP-70 | RP-152168 | 0563 |  |  | Introduction of intra-band CA\_8B to TS 36.307 | 12.10.0 |
| 12-2015 | RP-70 | RP-152164 | 0568 |  |  | Introduction of 3DL/2UL inter-band CA combinations with self-interference issues | 12.10.0 |
| 12-2015 | RP-70 | RP-152171 | 0579 |  |  | Introduction of Band 65 | 12.10.0 |
| 12-2015 | RP-70 | RP-152133 | 0592 |  |  | [Rel-12] Introduction of dual uplink CA into 36.307 | 12.10.0 |
| 12-2015 | RP-70 | RP-152164 | 0594 |  |  | Introduction of 3DL/2UL Inter-band CA for CA\_39A-41C and CA\_39C-41A | 12.10.0 |
| 12-2015 | RP-70 | RP-152166 | 0595 |  |  | Introduction of 3DL/3UL Inter-band CA for CA\_39A-41C and CA\_39C-41A | 12.10.0 |
| 12-2015 | RP-70 | RP-152163 | 0597 |  |  | Introduction of 5DL/1UL CA combinations into TS 36.307 (Rel-12) | 12.10.0 |
| 12-2015 | RP-70 | RP-152164 | 0600 |  |  | Introduction of 3DL/2UL inter-band CA\_3A-7A-28A in TS36.307 Rel-12 | 12.10.0 |
| 12-2015 | RP-70 | RP-152162 | 0603 |  |  | Introduction of finished 4DL inter-band CAs to TS 36.307 | 12.10.0 |
| 12-2015 | RP-70 | RP-152170 | 0606 |  |  | Introduction of CA\_7A-7A BCS1 to TS 36.307 | 12.10.0 |
| 12-2015 | RP-70 | RP-152173 | 0611 |  |  | Introduction of 1447-1467MHz Band into 36.307 | 12.10.0 |
| 12-2015 | RP-70 | RP-152156 | 0615 |  |  | Rel-13 2DL combinations | 12.10.0 |
| 12-2015 | RP-70 | RP-152161 | 0619 |  |  | Rel-13 3DL combinations | 12.10.0 |
| 12-2015 | RP-70 | RP-152172 | 0627 |  |  | Introduction of Band 66 | 12.10.0 |
| 12-2015 | RP-70 | RP-152159 | 0631 |  |  | Introduction of intra-band non-contiguous CA in Band 41 for 4DL | 12.10.0 |
| 12-2015 | RP-70 | RP-152165 | 0633 |  |  | Introduction of 2 UL and 3 DL mixed inter/intra cases without MSD into 36.307 Rel-12 | 12.10.0 |
| 12-2015 | RP-70 | RP-152167 | 0637 |  |  | Introduction of intra-band CA\_5B to TS 36.307 | 12.10.0 |
| 12-2015 | RP-70 | RP-152169 | 0639 |  |  | Introduction of intra-band non-contiguous CA in Band 5 | 12.10.0 |
| 03/2016 | RP-71 | RP-160480 | 0654 |  | B | Rel-13 3DL combinations | 12.11.0 |
| 03/2016 | RP-71 | RP-160481 | 0641 |  | B | Introduction of completed R13 4DL inter-band CAs to TS 36.307 | 12.11.0 |
| 03/2016 | RP-71 | RP-160482 | 0650 |  | B | Introduction of 5DL/1UL CA combinations into TS 36.307 (Rel-12) | 12.11.0 |
| 03/2016 | RP-71 | RP-160483 | 0646 |  | B | Introduction of Band 68 | 12.11.0 |
| 2016/06 | RP-72 | RP-161141 | 0681 | 1 | F | CR TS 36.307 REL-12 | 12.12.0 |
| 2016/06 | RP-72 | RP-161141 | 0690 | 1 | F | Correction of RRM multiple uplink requirements and test cases in 36.307 | 12.12.0 |
| 09/2016 | RP-73 | RP-161628 | 0694 |  | A | Release 12 36.307 CAT A CR to make Band 41 power class 2 release independent | 12.13.0 |
| 09/2016 | RP-73 | RP-161784 | 0702 |  | F | Correction of REL-12 TS 36.307 references | 12.13.0 |
| 12/2016 | RP-74 | RP-162398 | 0709 | 1 | B | Addition of CA bandwidth Class F | 12.14.0 |
| 12/2016 | RP-74 | RP-162420 | 0714 | 1 | F | Correction to UE category applicability | 12.14.0 |
| 12/2016 | RP-74 | RP-162390 | 0719 |  | F | Addition of UE category 0 to release independence specification | 12.14.0 |
| 06/2017 | RP-76 | RP-171291 | 0747 | 1 | F | Cleanup of TS 36.307 | 12.15.0 |
| 2018-03 | RAN#79 | RP-180288 | 4368 |  | B | Addition of missing features for TS 36.307 REL-12 | 12.16.0 |
| 2018-03 | RAN#79 | RP-180276 | 4373 |  | B | Introduction of 4UL CA into TS36.307 | 12.16.0 |
| 2018-06 | RAN#80 | RP-181108 | 4378 |  | B | TS 36.307 Rel-12 | 12.17.0 |
| 2018-06 | RAN#80 | RP-181097 | 4384 | 1 | A | TS 36.307 big CR for introduction new band support for 4Rx antenna ports R12 | 12.17.0 |
| 2018-06 | RAN#80 | RP-181095 | 4397 |  | B | Introduction of 3UL CA into TS36.307 | 12.17.0 |